{"text_format":"1","workbook":"xlsx","n_sheets":20,"sheets":["About","Index","Table A","Table B","Table C","Table D","Table E","Table F","Table G","Table H","Table I","Table J","Table K","Table L","Table M","Table N","Table O","Table P","Figure 5 - NP","Stacked DER-BTM"],"not_rendered":{"charts":84,"images":0,"macros":1,"external_links":2,"defined_names":1032,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"About","index":0,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[]
[null,"The tables in this workbook are published to provide additional details and summaries of data collected by NERC for the 2022 Long-Term Reliability Assessment (LTRA). See the 2022 LTRA Report published on the NERC Reliability Assessments page for information, definitions, and methods used by NERC. "]
[null,"NERC Reliability Assessments: https://www.nerc.com/pa/RAPA/ra/Pages/default.aspx"]
[]
[null,"For questions about this workbook or the 2022 LTRA email assessments@nerc.net"]

{"sheet":"Index","index":1,"n_rows":23,"n_cols":4,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[null,"Tab","Worksheet Name","Description"]
[null,"Table A","On-Peak BPS Generation Capacity","Existing and Developing Generation Capacity by Fuel Type"]
[null,"Table B","Wind, Solar, Battery, and Hybrid Resources by Assessment Area","Cumulative wind, solar, battery, and hybrid resources by Assessment Area through 2032"]
[]
[null,"Table C","Yearly Confirmed Retirements ","Cumulative confirmed retirements by fuel type through 2032"]
[]
[null,"Table D","Cumulative Behind-the-Meter Solar PV Growth","Cumulative BTM Solar PV Growth (MW) across all North America Assessment Areas through 2032"]
[null,"Table E","Existing and Developing BTM Solar PV","Existing and Developing BTM Solar PV (MW) by Assessment Area"]
[null,"Table F","10-year peak demand Projections and CAGR","10-year BPS aggregate summer and winter peak demand compound annual growth rates"]
[null,"Table G","10-year Net Energy for Load Projections and GAGR","10-year BPS aggregate NEL Projections and compound annual growth rates"]
[null,"Table H","Peak Demand Growth Rate By Assessment Area","10-year Summer and Winter Peak Demand CAGR for each Assessment Area"]
[null,"Table I","10-year Generation Fuel Mix On-Peak Capacity Change by Interconnection","Generation Fuel Mix On-Peak Capacity by Interconnection for 2022 and 2032 "]
[null,"Table J","10-year Generation Fuel Mix Installed (Nameplate) Capacity Change by Interconnection","Generation Fuel Mix Installed (Nameplate) Capacity by Interconnection for 2022 and 2032 "]
[null,"Table K","Future Cumulative Transmission Circuit Miles > 100 kV by Project Status","Projections of transmission projects over 100 kV by project status (under construction, planned, and conceptual)"]
[null,"Table L","Future Transmission Circuit Miles > 100kV by Voltage Class\n","Future transmission circuit miles by voltage class for each year from 2022-2032"]
[null,"Table M","Line Miles Projected through 2032 by Circuit Miles and Line Length in Miles\n","Projections for each assessment area for each year from 2022-2032"]
[null,"Table N","Future Transmission Circuit Miles by Primary Driver\n","Future transmission circuit miles by primary driver for each year from 2022-2032\n"]
[null,"Table O","Exisiting BPS Wind and Solar Generation Resources by Assessment Area","Existing BPS wind and solar generation installed and on-peak contribution by Assessment Area (Year 2022)"]
[null,"Table P","Demand Response","Demand Response Capacity for Year 1 and Year 5 by Assessment Area"]

{"sheet":"Table A","index":2,"n_rows":172,"n_cols":12,"rows_kept":172,"cut":false,"hidden":false,"merged":[[117,0,117,11],[136,0,136,11],[155,0,155,11],[3,0,3,11],[22,0,22,11],[41,0,41,11],[60,0,60,11],[79,0,79,11],[98,0,98,11]]}
[]
[null,null,"See Demand Assumptions and Resource Categories description in the 2022 LTRA for definitions of generating unit status tiers"]
[]
["Existing"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",201841.5294264862,197085.41892876328,191928.95264276318,189198.96505646454,184825.11595846454,180657.49035846454,174954.75120841875,169686.16643748671,166815.3463914867,166823.03717162684,162900.06849962688]
["Petroleum",34138.759881000042,33359.446618000024,33370.803714000023,33209.142569000054,33038.14256900004,32848.04256900007,32848.04256900007,32846.074923000037,32672.474923000053,32618.468672000025,32618.468672000025]
["Natural Gas and Other Gases",476783.52297320031,475146.24341853446,471160.20270773512,468256.67429473362,466632.85091473407,462268.25376873394,459973.45008873451,459811.57592753385,459324.31080753385,457978.22061053349,457749.43693053268]
["Biomass",7535.7295469999908,7519.8734980000027,7455.1271860000088,7387.1680770000075,7377.1847300000054,7243.8949500000053,7143.2794580000009,7022.4720640000014,6990.0256779999945,6988.8311049999929,6988.380824999992]
["Solar",39714.999494600066,39518.031089400029,38900.644258200075,38257.888963400066,38245.399099400071,38140.048939400076,37707.381419200086,38799.904308200064,38845.834228200081,38163.519237400062,37993.899029400069]
["Wind",29826.243399072027,28564.45664807201,28113.58128807199,28453.571562072011,28372.66277510607,28367.166275106076,28657.293460106088,27893.407566106071,27582.326496106096,27961.467110106096,28024.80485010608]
["Geothermal",4202.2568820000015,4198.9364360000009,4201.7246550000009,4203.7446160000018,4188.2525160000014,4188.2525160000014,4188.2525160000014,4161.2777889999998,4161.2777889999998,4167.4837700000026,4167.4837700000026]
["Conventional Hydro",114345.23231628638,114248.06741450574,111726.51266692771,110923.91637328772,110723.59651102542,111517.73661539801,112660.57062704726,111612.52061462415,112448.09588854889,111354.53592939394,111343.31592939392]
["Run of River Hydro",1702.5660000000028,1702.5660000000028,1702.5660000000028,1702.5660000000028,1702.5660000000028,1592.5660000000007,1592.5660000000007,1592.5660000000007,1592.5660000000007,1577.3480000000006,1569.3480000000006]
["Pumped Storage",20809.745006210276,20834.950494882069,20031.3896990229,20012.498911815157,20012.498911815157,20012.498911815157,20752.626179428666,20031.3896990229,20031.3896990229,20012.498911815157,20012.498911815157]
["Nuclear",106176.55636910725,104553.93356743566,106246.63457083005,104216.25267083006,103118.98767083006,101892.98767083006,101845.98767083006,101840.2944783226,102658.2944783226,101895.6832783226,101895.6832783226]
["Hybrid",430.702,430.63810000000001,430.29250000000002,430.33500000000004,430.33500000000004,430.33500000000004,430.33500000000004,430.63340000000005,430.63340000000005,430.8759,430.8759]
["Other",3222.9069080000004,3197.7845600000014,3197.5078290000006,3175.7297610000001,3161.0159000000003,3157.0819100000008,3157.2123640000009,3144.3498810000006,3144.4915879999999,3145.3127180000001,3145.2060580000011]
["Battery",2757.9601799999987,2757.3200369999995,2756.1744400000002,2756.0800000000004,2756.145,2756.0650000000001,2756.1650000000004,2757.6760629999985,2757.7160629999985,2757.6804429999984,2757.5604429999985]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Tier 1"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,0,0,0,0,0,0,0]
["Petroleum",0,0,0,0,0,0,0,0,0,0,0]
["Natural Gas and Other Gases",2623.962419404907,12741.679207788296,19747.743149505051,23412.660284505044,24497.807384505038,26560.475684505043,29312.009684505047,32699.507149505029,33390.350749505022,33905.965239505014,36198.524439504989]
["Biomass",48.659066000000003,114.5772798,114.51844200000001,114.51844200000001,114.51844200000001,114.51844200000001,114.51844200000001,114.55147220000002,114.55147220000002,114.55147220000002,114.55147220000002]
["Solar",4185.6806460000007,30785.784972000001,52544.394985496416,55489.039475496458,56203.903175496445,56769.553075496435,57117.93182149643,58085.671685496403,58303.454685496392,57734.636125496436,57646.452075496432]
["Wind",3135.0756879999999,6365.4554779999999,8301.916197999999,12330.327268000001,12801.500868000001,13079.135908,13104.598848,13079.648198000001,12963.780038000001,13030.789027999999,13079.135908]
["Geothermal",60.072199999999995,470.11220000000003,470.38660000000004,470.57024999999999,470.57024999999999,470.57024999999999,470.57024999999999,470.81574999999998,470.81574999999998,473.84840000000003,473.84840000000003]
["Conventional Hydro",294.08536955433988,712.1120707891223,1230.5337938751134,1357.6131245896659,1379.4954154987568,1538.2833297524039,1541.9984927472428,1526.3632366895995,1600.2433390465008,1600.8149390465003,1600.8149390465003]
["Run of River Hydro",0,0,0,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003]
["Pumped Storage",125.33923273657288,141.19741687979541,141.19741687979541,135.3948337595908,135.3948337595908,135.3948337595908,125.33923273657288,141.19741687979541,141.19741687979541,135.3948337595908,135.3948337595908]
["Nuclear",0,2200,2200,2200,2200,2200,2200,2200,2200,2200,2200]
["Hybrid",475.72500000000002,2114.5712000000003,2611.5138000000002,2610.1277,2610.1277,2610.1277,2610.1277,2612.155400000001,2612.155400000001,2612.4099000000006,2612.4099000000006]
["Other",0,695,755,755,755,755,755,755,755,755,755]
["Battery",1304.7189519999999,2827.0460119999998,3986.5521160000003,5035.7884809999996,5040.7884809999996,5395.7884809999996,6230.7884809999987,6920.303555999998,7561.295055999999,8109.737556,8471.8780559999996]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Tier 2"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,20,20,20,20,20,20,20]
["Petroleum",0,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571]
["Natural Gas and Other Gases",146.53200197219849,5832.6467155230293,11687.366655036078,12851.958975036081,16043.487204172559,18334.487204172561,18392.687204172562,18584.356964172559,19313.356964172559,19312.163324172569,19312.163324172569]
["Biomass",0,6,6,6,6,6,6,6,6,6,6]
["Solar",160.40463863372804,28806.670927358125,88729.040027861673,123470.36410005073,150361.17410005076,152334.71410005071,152421.87806605073,152609.64362805063,152631.38862805063,152455.3996000507,152468.90410005071]
["Wind",200,3600.2376320000003,7040.3099320000019,8420.8911320000025,12713.929482000007,13585.154482000007,16035.357174000001,16023.041982000002,16400.341982000002,16402.014482000002,16402.014482000002]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",0,533.62500076293941,637.58227123224788,640.53713854737441,640.49947213011546,790.77453809844064,783.13393839772982,827.993338697019,828.27453809844064,790.77453809844064,790.77453809844064]
["Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0]
["Pumped Storage",0,0,0,0,0,0,0,0,0,0,0]
["Nuclear",37,37,37,37,37,37,37,322,322,322,322]
["Hybrid",9.9980001449584961,6330.2157001449568,16739.507000144957,21133.44170228119,33756.271702281199,34061.271702281199,34061.271702281199,34061.455702281201,34061.455702281201,34061.455702281201,34061.455702281201]
["Other",0,1515.7,2608.1100539463896,2858.0100539463892,3158.0100539463892,3158.0100539463892,3158.0100539463892,3158.0100539463892,3158.0100539463892,3158.0100539463892,3158.0100539463892]
["Battery",10,8225.1682999999994,16245.664293896485,25156.289772412107,27927.189772412108,28432.189772412108,29027.189772412108,29312.46807241211,29312.46807241211,29312.10057241211,29312.10057241211]
["Unknown",0,0,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56]
[]
[]
["Tier 3"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,0,0,0,0,0,0,0]
["Petroleum",0,58,58,58,98,98,98,98,98,98,98]
["Natural Gas and Other Gases",564,7168.6429800953674,14572.830070095368,18361.919320095374,19889.307870095363,21636.086170095368,21840.891170095358,22479.524394695378,23631.189574695352,23770.65827469535,23846.169874695392]
["Biomass",0,0,0,0,0,0,0,0,0,0,0]
["Solar",2451.2370000000001,13515.281159973145,25147.988659973147,43058.974523346922,50829.015022187246,52441.462722187243,54516.783454187251,56285.903678187242,58028.053178187241,67514.012522187229,68970.862522187221]
["Wind",450.11579999999998,3279.1623800000002,4983.9016200591277,5794.6129000591282,13025.099799965286,15924.715299965286,16404.282399965286,16823.84361996529,17072.796519965286,17939.401499965283,18064.823499965285]
["Geothermal",0,0,0,0,42.486400000000003,42.486400000000003,42.486400000000003,42.6096,42.6096,792.01259999999991,792.01259999999991]
["Conventional Hydro",0,0,0,0,0.55041526374859706,30.718039655817435,29.365099139543581,28.01215862326973,57.822192293303409,74.084683875794994,74.084683875794994]
["Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0]
["Pumped Storage",0,0,0,0,0,0,0,0,0,220.61411346387041,220.61411346387041]
["Nuclear",0,0,0,0,0,0,443.09999999999997,442.85,1093.73,1099.3799999999999,1099.3799999999999]
["Hybrid",0,529,836.57349999999997,2662.0888500000001,4608.6288530517577,5683.6288530517577,5799.8342030517579,6359.1581030517573,6968.392203051757,7869.9233530517577,7944.9233530517577]
["Other",958,3232.1,6435.5,8770.5,9170.5,10170.5,10170.5,10170.5,10170.5,10170.5,10170.5]
["Battery",0,364.39999389648438,1467.2600036621093,2873.4999787902834,3605.0684838104248,3996.8684868621826,4146.8684868621831,4295.9084868621831,4315.7724868621826,13182.897645862184,13182.777645862185]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing + Tier 1"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",201841.5294264862,197085.41892876328,191928.95264276318,189198.96505646454,184825.11595846454,180657.49035846454,174954.75120841875,169686.16643748671,166815.3463914867,166823.03717162684,162900.06849962688]
["Petroleum",34138.759881000042,33359.446618000024,33370.803714000023,33209.142569000054,33038.14256900004,32848.04256900007,32848.04256900007,32846.074923000037,32672.474923000053,32618.468672000025,32618.468672000025]
["Natural Gas and Other Gases",479407.48539260519,487887.92262632278,490907.94585724018,491669.33457923867,491130.65829923912,488828.72945323901,489285.45977323956,492511.08307703887,492714.6615570389,491884.18585003848,493947.96137003769]
["Biomass",7584.388612999991,7634.4507778000025,7569.6456280000084,7501.6865190000071,7491.703172000005,7358.4133920000049,7257.7979000000005,7137.0235362000012,7104.5771501999943,7103.3825771999927,7102.9322971999918]
["Solar",43900.680140600067,70303.816061400023,91445.03924369649,93746.928438896517,94449.302274896516,94909.602014896518,94825.313240696516,96885.575993696461,97149.28891369648,95898.155362896505,95640.351104896501]
["Wind",32961.319087072028,34929.912126072013,36415.497486071989,40783.898830072008,41174.163643106069,41446.302183106076,41761.892308106086,40973.055764106073,40546.106534106097,40992.256138106095,41103.94075810608]
["Geothermal",4262.3290820000011,4669.0486360000014,4672.1112550000007,4674.3148660000015,4658.8227660000011,4658.8227660000011,4658.8227660000011,4632.0935389999995,4632.0935389999995,4641.3321700000024,4641.3321700000024]
["Conventional Hydro",114639.31768584071,114960.17948529487,112957.04646080283,112281.52949787739,112103.09192652417,113056.01994515042,114202.5691197945,113138.88385131376,114048.3392275954,112955.35086844044,112944.13086844042]
["Run of River Hydro",1702.5660000000028,1702.5660000000028,1702.5660000000028,1743.2660000000028,1743.2660000000028,1633.2660000000008,1633.2660000000008,1633.2660000000008,1633.2660000000008,1618.0480000000007,1610.0480000000007]
["Pumped Storage",20935.084238946849,20976.147911761866,20172.587115902697,20147.893745574747,20147.893745574747,20147.893745574747,20877.965412165238,20172.587115902697,20172.587115902697,20147.893745574747,20147.893745574747]
["Nuclear",106176.55636910725,106753.93356743566,108446.63457083005,106416.25267083006,105318.98767083006,104092.98767083006,104045.98767083006,104040.2944783226,104858.2944783226,104095.6832783226,104095.6832783226]
["Hybrid",906.42700000000002,2545.2093000000004,3041.8063000000002,3040.4627,3040.4627,3040.4627,3040.4627,3042.7888000000012,3042.7888000000012,3043.2858000000006,3043.2858000000006]
["Other",3222.9069080000004,3892.7845600000014,3952.5078290000006,3930.7297610000001,3916.0159000000003,3912.0819100000008,3912.2123640000009,3899.3498810000006,3899.4915879999999,3900.3127180000001,3900.2060580000011]
["Battery",4062.6791319999984,5584.3660489999993,6742.7265560000005,7791.8684809999995,7796.933481,8151.8534810000001,8986.9534809999986,9677.9796189999961,10319.011118999997,10867.417998999998,11229.438498999998]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing + Tier 1 + Tier 2"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",201841.5294264862,197085.41892876328,191928.95264276318,189198.96505646454,184845.11595846454,180677.49035846454,174974.75120841875,169706.16643748671,166835.3463914867,166843.03717162684,162920.06849962688]
["Petroleum",34138.759881000042,33383.888651252943,33395.245747252942,33233.584602252973,33062.584602252959,32872.484602252989,32872.484602252989,32870.516956252955,32696.916956252968,32642.91070525294,32642.91070525294]
["Natural Gas and Other Gases",479554.01739457739,493720.56934184581,502595.31251227623,504521.29355427477,507174.14550341165,507163.21665741154,507678.14697741211,511095.44004121143,512028.01852121146,511196.34917421103,513260.12469421024]
["Biomass",7584.388612999991,7640.4507778000025,7575.6456280000084,7507.6865190000071,7497.703172000005,7364.4133920000049,7263.7979000000005,7143.0235362000012,7110.5771501999943,7109.3825771999927,7108.9322971999918]
["Solar",44061.084779233795,99110.486988758144,180174.07927155815,217217.29253894725,244810.47637494729,247244.31611494723,247247.19130674726,249495.21962174709,249780.67754174711,248353.55496294721,248109.2552049472]
["Wind",33161.319087072028,38530.149758072017,43455.807418071992,49204.789962072013,53888.093125106076,55031.456665106081,57797.249482106083,56996.097746106076,56946.448516106102,57394.270620106094,57505.955240106079]
["Geothermal",4262.3290820000011,4669.0486360000014,4672.1112550000007,4674.3148660000015,4658.8227660000011,4658.8227660000011,4658.8227660000011,4632.0935389999995,4632.0935389999995,4641.3321700000024,4641.3321700000024]
["Conventional Hydro",114639.31768584071,115493.80448605781,113594.62873203508,112922.06663642476,112743.59139865429,113846.79448324886,114985.70305819223,113966.87719001078,114876.61376569384,113746.12540653888,113734.90540653886]
["Run of River Hydro",1702.5660000000028,1702.5660000000028,1702.5660000000028,1743.2660000000028,1743.2660000000028,1633.2660000000008,1633.2660000000008,1633.2660000000008,1633.2660000000008,1618.0480000000007,1610.0480000000007]
["Pumped Storage",20935.084238946849,20976.147911761866,20172.587115902697,20147.893745574747,20147.893745574747,20147.893745574747,20877.965412165238,20172.587115902697,20172.587115902697,20147.893745574747,20147.893745574747]
["Nuclear",106213.55636910725,106790.93356743566,108483.63457083005,106453.25267083006,105355.98767083006,104129.98767083006,104082.98767083006,104362.2944783226,105180.2944783226,104417.6832783226,104417.6832783226]
["Hybrid",916.42500014495852,8875.4250001449582,19781.313300144957,24173.90440228119,36796.734402281203,37101.734402281203,37101.734402281203,37104.244502281203,37104.244502281203,37104.741502281198,37104.741502281198]
["Other",3222.9069080000004,5408.4845600000017,6560.6178829463897,6788.7398149463897,7074.0259539463896,7070.09196394639,7070.2224179463901,7057.3599349463893,7057.5016419463891,7058.3227719463894,7058.2161119463908]
["Battery",4072.6791319999984,13809.534348999998,22988.390849896485,32948.158253412104,35724.123253412108,36584.043253412106,38014.143253412105,38990.447691412104,39631.479191412109,40179.518571412103,40541.539071412109]
["Unknown",0,0,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56]
[]
[]
["Existing + Tier 1 + Tier 2 + Tier 3"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",201841.5294264862,197085.41892876328,191928.95264276318,189198.96505646454,184845.11595846454,180677.49035846454,174974.75120841875,169706.16643748671,166835.3463914867,166843.03717162684,162920.06849962688]
["Petroleum",34138.759881000042,33441.888651252943,33453.245747252942,33291.584602252973,33160.584602252959,32970.484602252989,32970.484602252989,32968.516956252955,32794.916956252971,32740.91070525294,32740.91070525294]
["Natural Gas and Other Gases",480118.01739457739,500889.21232194116,517168.1425823716,522883.21287437016,527063.45337350701,528799.30282750691,529519.03814750747,533574.96443590685,535659.20809590677,534967.00744890643,537106.29456890561]
["Biomass",7584.388612999991,7640.4507778000025,7575.6456280000084,7507.6865190000071,7497.703172000005,7364.4133920000049,7263.7979000000005,7143.0235362000012,7110.5771501999943,7109.3825771999927,7108.9322971999918]
["Solar",46512.321779233796,112625.76814873129,205322.06793153129,260276.26706229418,295639.49139713455,299685.77883713448,301763.97476093454,305781.12329993432,307808.73071993433,315867.56748513447,317080.11772713443]
["Wind",33611.434887072028,41809.312138072019,48439.709038131121,54999.402862131145,66913.192925071358,70956.171965071364,74201.531882071373,73819.941366071362,74019.245036071385,75333.67212007138,75570.778740071371]
["Geothermal",4262.3290820000011,4669.0486360000014,4672.1112550000007,4674.3148660000015,4701.3091660000009,4701.3091660000009,4701.3091660000009,4674.7031389999993,4674.7031389999993,5433.3447700000024,5433.3447700000024]
["Conventional Hydro",114639.31768584071,115493.80448605781,113594.62873203508,112922.06663642476,112744.14181391803,113877.51252290467,115015.06815733177,113994.88934863405,114934.43595798714,113820.21009041468,113808.99009041466]
["Run of River Hydro",1702.5660000000028,1702.5660000000028,1702.5660000000028,1743.2660000000028,1743.2660000000028,1633.2660000000008,1633.2660000000008,1633.2660000000008,1633.2660000000008,1618.0480000000007,1610.0480000000007]
["Pumped Storage",20935.084238946849,20976.147911761866,20172.587115902697,20147.893745574747,20147.893745574747,20147.893745574747,20877.965412165238,20172.587115902697,20172.587115902697,20368.507859038618,20368.507859038618]
["Nuclear",106213.55636910725,106790.93356743566,108483.63457083005,106453.25267083006,105355.98767083006,104129.98767083006,104526.08767083006,104805.1444783226,106274.02447832259,105517.0632783226,105517.0632783226]
["Hybrid",916.42500014495852,9404.4250001449582,20617.886800144955,26835.993252281191,41405.363255332959,42785.363255332959,42901.568605332963,43463.402605332958,44072.63670533296,44974.664855332958,45049.664855332958]
["Other",4180.9069080000008,8640.5845600000011,12996.11788294639,15559.23981494639,16244.52595394639,17240.59196394639,17240.722417946388,17227.859934946391,17228.00164194639,17228.82277194639,17228.716111946393]
["Battery",4072.6791319999984,14173.934342896482,24455.650853558593,35821.65823220239,39329.191737222536,40580.911740274292,42161.011740274291,43286.356178274291,43947.25167827429,53362.416217274287,53724.316717274298]
["Unknown",0,0,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56]
[]
["Existing"]
["Tier 1 + Tier 2"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,20,20,20,20,20,20,20]
["Petroleum",0,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571,24.442033252915571]
["Natural Gas and Other Gases",2770.4944213771055,18574.325923311328,31435.109804541127,36264.619259541127,40541.2945886776,44894.962888677604,47704.696888677609,51283.864113677584,52703.707713677577,53218.128563677586,55510.687763677561]
["Biomass",48.659066000000003,120.5772798,120.51844200000001,120.51844200000001,120.51844200000001,120.51844200000001,120.51844200000001,120.55147220000002,120.55147220000002,120.55147220000002,120.55147220000002]
["Solar",4346.0852846337284,59592.45589935813,141273.43501335807,178959.40357554719,206565.0772755472,209104.26717554714,209539.80988754716,210695.31531354703,210934.84331354703,210190.03572554715,210115.35617554715]
["Wind",3335.0756879999999,9965.6931100000002,15342.226130000001,20751.218400000005,25515.43035000001,26664.290390000009,29139.956021999998,29102.690180000005,29364.122020000003,29432.803510000002,29481.150390000003]
["Geothermal",60.072199999999995,470.11220000000003,470.38660000000004,470.57024999999999,470.57024999999999,470.57024999999999,470.57024999999999,470.81574999999998,470.81574999999998,473.84840000000003,473.84840000000003]
["Conventional Hydro",294.08536955433988,1245.7370715520617,1868.1160651073612,1998.1502631370404,2019.9948876288722,2329.0578678508446,2325.1324311449725,2354.3565753866187,2428.5178771449414,2391.5894771449412,2391.5894771449412]
["Run of River Hydro",0,0,0,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003]
["Pumped Storage",125.33923273657288,141.19741687979541,141.19741687979541,135.3948337595908,135.3948337595908,135.3948337595908,125.33923273657288,141.19741687979541,141.19741687979541,135.3948337595908,135.3948337595908]
["Nuclear",37,2237,2237,2237,2237,2237,2237,2522,2522,2522,2522]
["Hybrid",485.72300014495852,8444.7869001449581,19351.020800144957,23743.569402281191,36366.399402281197,36671.399402281197,36671.399402281197,36673.611102281204,36673.611102281204,36673.865602281199,36673.865602281199]
["Other",0,2210.6999999999998,3363.1100539463896,3613.0100539463892,3913.0100539463892,3913.0100539463892,3913.0100539463892,3913.0100539463892,3913.0100539463892,3913.0100539463892,3913.0100539463892]
["Battery",1314.7189519999999,11052.214312,20232.216409896486,30192.078253412106,32967.978253412104,33827.978253412104,35257.978253412104,36232.771628412105,36873.763128412109,37421.838128412113,37783.978628412107]
["Unknown",0,0,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56]
[]
[]
["Tier 1 + Tier 2 + Tier 3"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,20,20,20,20,20,20,20]
["Petroleum",0,82.442033252915564,82.442033252915564,82.442033252915564,122.44203325291556,122.44203325291556,122.44203325291556,122.44203325291556,122.44203325291556,122.44203325291556,122.44203325291556]
["Natural Gas and Other Gases",3334.4944213771055,25742.968903406694,46007.939874636497,54626.538579636501,60430.602458772963,66531.049058772973,69545.588058772963,73763.388508372969,76334.897288372929,76988.786838372936,79356.857638372952]
["Biomass",48.659066000000003,120.5772798,120.51844200000001,120.51844200000001,120.51844200000001,120.51844200000001,120.51844200000001,120.55147220000002,120.55147220000002,120.55147220000002,120.55147220000002]
["Solar",6797.3222846337285,73107.737059331281,166421.42367333121,222018.37809889411,257394.09229773446,261545.72989773439,264056.59334173443,266981.21899173426,268962.89649173425,277704.04824773438,279086.21869773435]
["Wind",3785.1914879999999,13244.85549,20326.127750059128,26545.831300059133,38540.5301499653,42589.005689965299,45544.238421965289,45926.533799965298,46436.918539965292,47372.205009965284,47545.973889965288]
["Geothermal",60.072199999999995,470.11220000000003,470.38660000000004,470.57024999999999,513.05664999999999,513.05664999999999,513.05664999999999,513.42534999999998,513.42534999999998,1265.8609999999999,1265.8609999999999]
["Conventional Hydro",294.08536955433988,1245.7370715520617,1868.1160651073612,1998.1502631370404,2020.5453028926208,2359.775907506662,2354.497530284516,2382.3687340098886,2486.3400694382449,2465.6741610207359,2465.6741610207359]
["Run of River Hydro",0,0,0,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003]
["Pumped Storage",125.33923273657288,141.19741687979541,141.19741687979541,135.3948337595908,135.3948337595908,135.3948337595908,125.33923273657288,141.19741687979541,141.19741687979541,356.00894722346118,356.00894722346118]
["Nuclear",37,2237,2237,2237,2237,2237,2680.1,2964.85,3615.73,3621.38,3621.38]
["Hybrid",485.72300014495852,8973.7869001449581,20187.594300144956,26405.658252281191,40975.028255332953,42355.028255332953,42471.233605332956,43032.769205332959,43642.003305332961,44543.788955332959,44618.788955332959]
["Other",958,5442.7999999999993,9798.6100539463896,12383.510053946389,13083.510053946389,14083.510053946389,14083.510053946389,14083.510053946389,14083.510053946389,14083.510053946389,14083.510053946389]
["Battery",1314.7189519999999,11416.614305896484,21699.476413558594,33065.578232202388,36573.046737222532,37824.84674027429,39404.84674027429,40528.680115274285,41189.53561527429,50604.735774274297,50966.756274274288]
["Unknown",0,0,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56,7.56]

{"sheet":"Table B","index":3,"n_rows":83,"n_cols":30,"rows_kept":83,"cut":false,"hidden":false,"merged":[[60,1,60,5],[59,0,59,5],[4,1,4,5],[4,6,4,10],[3,0,3,10],[31,0,31,10],[32,1,32,5],[32,6,32,10]]}
[]
[null,null,null,null,"See Demand Assumptions and Resource Categories description in the 2022 LTRA for definitions of generating unit status tiers"]
[]
[" Solar and Wind Nameplate Capacity, Existing and Planned Additions through 2032"]
[null,"Nameplate MW of Solar",null,null,null,null,"Nameplate MW of Wind"]
[null,"Existing","Tier 1","Tier 2","Tier 3","Total","Existing","Tier 1","Tier 2","Tier 3","Total",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"How do we cut off?"]
["MISO",1768.65,9544.08,86407.080000000016,10481,108200.81000000001,26067.992000000002,2840.4,17345.849999999999,5405.9,51660.142]
["MRO-Manitoba",0,0,0,0,0,258.5,0,0,0,258.5]
["MRO-SaskPower",25.599999999999998,20,0,121.9,167.5,626.6,200,0,0,826.6]
["NPCC-Maritimes",10.24,99.02,31,13.1,153.35999999999999,1210.4000000000001,370,0,505,2085.4]
["NPCC-New England",2315.9506999999971,444.19999885559082,1388.2609956741333,1570.3419952392578,5718.7536897689788,1503.8163999999995,2324,10504.5,4500.8499994277954,18833.166399427795]
["NPCC-New York",51.5,1273.3,3667.8,2170,7162.6,1897.3000000000002,791.9,6927.5,5042.2000000000007,14658.900000000001]
["NPCC-Ontario",478,0,0,0,478,4783.0119999999988,159.76,0,0,4942.771999999999]
["NPCC-Quebec",9.5,0,0,0,9.5,3715.7499999999995,204,0,0,3919.7499999999995]
["PJM",4988.473,14470.084999999994,96862.797000000006,0,116321.355,11013.2,5402.86,31704.279999999995,0,48120.34]
["SERC-C",449.77999999999992,1828.2,380,6000,8657.98,964.4,0,0,0,964.4]
["SERC-E",726.53,130,0,0,856.53,0,0,0,0,0]
["SERC-FP",5544.5599999999995,10946.929999999998,0,0,16491.489999999998,0,0,0,0,0]
["SERC-SE",3775.3899999999994,3863.7999999999997,799.6,4013.83,12452.619999999999,0,0,0,0,0]
["SPP",393.77999999999992,2300,0,25500,28193.78,30264.3,8200,1175,12500,52139.3]
["Texas RE-ERCOT",11603.1,27754.879999999994,56609.02,19451.179999999997,115418.18,35690.33,5758.5,6110.3099999999995,3357,50916.14]
["WECC-AB",336,736.5,0,350,1422.5,2269,1369.6,0,1600,5238.6000000000004]
["WECC-BC",2.04,15,15,0,32.04,717,0,0,15,732]
["WECC-CA/MX",17010.701999999994,4962.5599999999995,60,12914,34947.261999999995,8828.25,243.2,486.28,4005,13562.730000000001]
["WECC-WPP",6315.3189999999959,8034.76,1981.99,3362.48,19694.548999999995,18564.179999999993,1101.3,75,3874.8,23615.279999999992]
["WECC-SRSG",2427.5980000000004,2917.7,650,4406,10401.298000000001,1800.6100000000001,1843.8200000000002,203,135,3982.4300000000003]
["Total",58232.712699999982,89341.014998855564,248852.54799567413,90353.831995239248,486780.10768976895,150174.64039999997,30809.339999999997,74531.719999999987,40940.749999427797,296456.45039942779]
[]
[]
[]
[]
[" Hybrid Solar and Hybrid Wind Nameplate Capacity, Existing and Planned Additions through 2032"]
[null,"Nameplate MW of Solar",null,null,null,null,"Nameplate MW of Wind"]
[null,"Existing","Tier 1","Tier 2","Tier 3","Total","Existing","Tier 1","Tier 2","Tier 3","Total"]
["MISO",0,0,4270,525,4795,0,0,0,0,0]
["MRO-Manitoba",0,0,0,0,0,0,0,0,0,0]
["MRO-SaskPower",0,0,0,0,0,0,0,0,0,0]
["NPCC-Maritimes",0,0,0,0,0,0,0,0,0,0]
["NPCC-New England",75.839800000000011,0,123.00800228118896,348.30000305175781,547.14780533294675,0,0,0,0,0]
["NPCC-New York",0,0,0,0,0,0,0,0,0,0]
["NPCC-Ontario",0,0,0,0,0,0,0,0,0,0]
["NPCC-Quebec",0,0,0,0,0,0,0,0,0,0]
["PJM",2.9,1963.7720000000002,29116.896000000004,0,31083.568000000003,0,90,199,0,289]
["SERC-C",0,0,0,0,0,0,0,0,0,0]
["SERC-E",0,0,0,0,0,0,0,0,0,0]
["SERC-FP",0,0,0,0,0,0,0,0,0,0]
["SERC-SE",0,0,0,0,0,0,0,0,0,0]
["SPP",0,0,0,0,0,0,0,0,0,0]
["Texas RE-ERCOT",0,0,0,0,0,0,0,0,0,0]
["WECC-AB",0,0,0,0,0,0,0,0,0,0]
["WECC-BC",0,0,0,0,0,0,0,0,0,0]
["WECC-CA/MX",403,696,230,0,1329,0,0,0,0,0]
["WECC-WPP",25,548,0,2335.5,2908.5,0,0,0,160,160]
["WECC-SRSG",0,160,0,0,160,0,0,0,0,0]
["Total",506.7398,3367.7719999999999,33739.904002281197,3208.8000030517578,40823.215805332948,0,90,199,160,449]
[]
[]
[]
[]
[" Battery Nameplate Capacity, Existing and Planned Additions through 2032"]
[null,"Nameplate MW of Battery"]
[null,"Existing","Tier 1","Tier 2","Tier 3","Total"]
["MISO",0,0,0,0,0]
["MRO-Manitoba",0,0,0,0,0]
["MRO-SaskPower",0,0,0,0,0]
["NPCC-Maritimes",0,0,200,0,200]
["NPCC-New England",47.141317999999998,325,3042.1799791259764,3392.3259868621826,6806.647283988159]
["NPCC-New York",0,0,0,0,0]
["NPCC-Ontario",7.7,0,250,0,257.7]
["NPCC-Quebec",0,0,0,0,0]
["PJM",0,110.69999999999999,32013.08,0,32123.780000000002]
["SERC-C",0,246,20,700,966]
["SERC-E",23.85,0,0,0,23.85]
["SERC-FP",508.3,3460.8,0,0,3969.1000000000004]
["SERC-SE",0,1.5,0,0,1.5]
["SPP",0,0,0,0,0]
["Texas RE-ERCOT",2298.4299999999998,5333.6,42432.630000000005,19808.71,69873.37]
["WECC-AB",50,0,0,50,100]
["WECC-BC",0,0,0,0,0]
["WECC-CA/MX",2233.56,2610.6099999999997,344,9367.89,14556.06]
["WECC-WPP",12.4,1385,75,245,1717.4]
["WECC-SRSG",40.799999999999997,1888.5,290,0,2219.3000000000002]
["Total",5222.1813179999999,15361.71,78666.88997912599,33563.925986862181,132814.70728398813]

{"sheet":"Table C","index":4,"n_rows":7,"n_cols":13,"rows_kept":7,"cut":false,"hidden":false,"merged":[[1,0,1,12]]}
[]
["Confirmed Retirements from 2012 to 2032"]
[null,"2012-2021",2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Nuclear",2147.6999999999998,0,0,2180,3330,5394,5394,5394,5394,6162.6,6162.6,6162.6]
["Coal",34406.400000000001,8623.5999999999985,15611.029999999999,18391.53,24606.23,29318.129999999997,34920.136335877862,39550.096335877861,43712.87633587786,46484.87633587786,49905.816335877862,51398.416335877861]
["Natural Gas and Other Gases",10372.177999999998,3001.1499999999996,7429.8,11205.6,13327.900000000001,15804.86,21988.460000000003,22220.06,22720.940000000002,23627.340000000004,24966.340000000004,25794.630000000005]
["Biomass",932.25699999999995,27.988999999999997,58.069000000000003,130.79699999999997,271.54699999999997,323.64699999999999,411.24699999999996,510.04699999999997,510.04699999999997,545.04700000000003,545.04700000000003,558.64700000000005]

{"sheet":"Table D","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Table E","index":6,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,"Existing","2023 (S)","2024 (S)","2025 (S)","2026 (S)","2027 (S)","2028 (S)","2029 (S)","2030 (S)","2031 (S)","2032 (S)","Planned"]
["MISO",861,861,861,861,861,861,861,861,861,861,861,0]
["MRO-Manitoba",37.6,39.799999999999997,42,44.287840750000001,47.047959550886198,50.376201833676802,54.387111199688661,59.217232692323051,65.028839998365683,72.014062548563501,80.400000000000006,42.800000000000004]
["MRO-SaskPower",36,39,42,45,48,51,51,51,51,51,51,15]
["NPCC-Maritimes",69.766739362876336,90.672519966648238,109.16480684378509,126.10337329119322,145.83404359531727,169.98355360230761,198.13311156213189,231.00428769003841,268.89335990349497,302.91764867286224,326.99265541172912,257.22591604885281]
["NPCC-New England",3146,3500,3870,4239,4669,5009,5333,5648,5948,6244,6555,3409]
["NPCC-New York",3896,4710.5,5611.5,6498.5,7333,8119.9999999999991,8831,9433.5,9886.5,10185,10393,6497]
["NPCC-Ontario",2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999949,2189.6217474999958,2189.6217474999921,2189.6217474999903,2189.6217474999917,0]
["NPCC-Quebec",16,42,78,125,181,244,313,386,473,576,576,560]
["PJM",8289.4736842105267,9205.2631578947367,10055.263157894737,10615.78947368421,11115.78947368421,12228.947368421053,12802.631578947368,13547.368421052632,14847.368421052632,15721.052631578947,17639.473684210527,9350]
["SERC-C",49,49,49,49,49,49,49,49,49,49,49,0]
["SERC-E",549,636,710,774,840,907,975,1045,1116,1187,1258,709]
["SERC-FP",1125,1492,1806,2066,2328,2601,2921,3276,3695,4051,4365,3240]
["SERC-SE",0,0,0,0,0,0,0,0,0,0,0,0]
["SPP",62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,0]
["Texas RE-ERCOT",1531.2368612250004,2031.2368612250004,2531.2368612250002,3031.2368612250002,3531.2368612250002,4031.2368612250007,4531.2368612250002,5031.2368612250002,5531.2368612250002,6031.2368612250002,6531.2368612250002,5000]
["WECC-AB",115,128,142,155,192,228,264,300,336,396,456,341]
["WECC-BC",0,0,0,0,0,0,0,0,0,0,0,0]
["WECC-CA/MX",7785.72757453136,8940.9092136122727,10038.88160020766,11048.351492423804,12096.902862861947,13170.567137112188,14232.328309451304,15393.043798843171,16597.839475193981,17788.831598533237,18929.873721872485,11144.146147341125]
["WECC-WPP",2775.5878322637027,3057.1534160558031,3297.8327191715562,3524.7008736571538,3758.1386215531033,4006.9149011708023,4275.5496489824754,4570.1888949760714,4885.5804218445201,5196.1301782279934,3975.4294830158901,1199.8416507521874]
["WECC-SRSG",1971.2936324069678,2160.4248702960317,2404.8008925386421,2701.9200983278606,3059.0647430940999,3479.0412510163706,3965.4778916417135,4516.2002616477412,5135.926559655144,5825.0391233269747,6586.9727702563196,4615.6791378493517]

{"sheet":"Table F","index":7,"n_rows":38,"n_cols":14,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["LTRA","Assessment Period","First Year Summer (MW)","Last Year Summer (MW)","First Year Winter (MW)","Last Year Winter (MW)","10–Year Summer Growth (MW)","10–Year Winter Growth (MW)","Total Summer Growth (%)","Total Winter Growth (%)","Summer CAGR (%)","Winter CAGR (%)"]
[1990,"1990–99",596358,716323,569126,688501,119965,119375,0.20116272440379773,0.20975144344134691,2.0574351266605229E-2,2.138261396582708E-2]
[1991,"1991–00",610112,722426,582626,695188,112314,112562,0.18408751180111194,0.19319769457593722,1.8952069355399503E-2,1.9820178049766213E-2]
[1992,"1992–01",622963,734586,591543,700506,111623,108963,0.17918078601778917,0.18420131757116559,1.848204491709482E-2,1.8962950464786354E-2]
[1993,"1993–02",631759,742316,597849,706754,110557,108905,0.17499869412228397,0.18216138188739966,1.8080060144674004E-2,1.8767768559400322E-2]
[1994,"1994–03",640983,746426,600092,702881,105443,102789,0.1645020226745483,0.1712887357271885,1.7065484895145255E-2,1.7722391139798788E-2]
[1995,"1995–04",660655,773122,616234,722968,112467,106734,0.17023559951865952,0.17320368561293276,1.7620677074857705E-2,1.7907132827500671E-2]
[1996,"1996–05",676984,790282,629030,730492,113298,101462,0.16735698332604612,0.16129914312512916,1.7342238661665066E-2,1.6754285854778228E-2]
[1997,"1997–06",693961,809767,644791,751212,115806,106421,0.16687681296211171,0.16504727888571646,1.7295734090776005E-2,1.7118387422509374E-2]
[1998,"1998–07",712516,833693,658318,766554,121177,108236,0.1700691633591386,0.16441294328880571,1.7604594882678626E-2,1.705684003167085E-2]
[1999,"1999–08",732907,859403,666954,778931,126496,111977,0.17259488584499807,0.16789313805749723,1.7848428936110716E-2,1.7394145238486924E-2]
[2000,"2000–09",752014,888553,678396,794906,136539,116510,0.18156443895991298,0.17174334754332277,1.8710596186560569E-2,1.7766273367664009E-2]
[2001,"2001–10",776367,921328,693831,817309,144961,123478,0.18671710672916289,0.17796552762848589,1.9203251076668204E-2,1.8365364463075906E-2]
[2002,"2002–11",779392,930714,694157,816144,151322,121987,0.19415390458203319,0.17573401982548617,1.9910953275390719E-2,1.8150832071895273E-2]
[2003,"2003–12",789078,941602,699389,821429,152524,122040,0.19329394559219748,0.17449516649532665,1.9829318307449162E-2,1.8031575069626271E-2]
[2004,"2004–13",800011,951140,703022,818730,151129,115708,0.18890865250602804,0.16458659899690195,1.9412212177339239E-2,1.7073692207044466E-2]
[2005,"2005–14",820699,972889,719526,839471,152190,119945,0.18543948512182906,0.16670002195890071,1.908127315405217E-2,1.7278607571412197E-2]
[2006,"2006–15",839135,990850,732209,847887,151715,115678,0.18079927544435639,0.15798494692089279,1.8637274881586174E-2,1.6431466840501674E-2]
[2007,"2007–16",862772,1005326,748592,856393,142554,107801,0.1652278933484165,0.14400501207600402,1.7135906371505083E-2,1.5060649380245428E-2]
[2008,"2008–17",863887.34,1002244.9029999999,751697.49,856163.86,138357.56299999997,104466.37,0.16015695171548638,0.13897395081098382,1.6643123380144065E-2,1.4563677814831477E-2]
[2009,"2009–18",855777,980224,738052.97038185014,831971.93724520481,124447,93918.966863354668,0.14541989326658697,0.12725233910347022,1.5200062268870163E-2,1.339819691898092E-2]
[2010,"2010–19",837551,950415,731189.58806559106,818072.99698480999,112864,86883.408919218928,0.13475477911195854,0.1188247348393931,1.414539857983188E-2,1.2553563845763449E-2]
["2011*","2011–21",849980.91739644052,960616.50675036653,760442.59370980063,844029.08411835565,110635.58935392601,83586.490408555022,0.13016243904958674,0.10991821223582489,1.3688550110104503E-2,1.1654763618323072E-2]
[2012,"2013–22*",862098.08137924364,973363.84433189163,760843.58325763582,848803.10015338799,111265.76295264799,87959.516895752167,0.12906392596842042,0.11560788423705143,1.300720989919868E-2,1.1151971524111626E-2]
[2013,"2014–23",868877.20264641545,970155.65563846449,771619.34585199133,848803.10015338787,101278.45299204905,77183.754301396548,0.1165624471255275,0.10002827782418197,1.2325869688292856E-2,1.064917942990018E-2]
[2014,"2015–24",864288.39420412143,950171.43358290044,767062.89009859413,837497.04897747654,85883.039378779009,70434.158878882416,9.9368497777717196E-2,9.1823186583604888E-2,1.058180904251893E-2,9.8087880113082448E-3]
[2015,"2016–25",865206.01596509153,945287.14896187885,765873.40128414705,831458.80011448555,80081.132996787317,65585.398830338498,9.255730024884426E-2,8.5634778176616203E-2,9.8842065105086974E-3,9.1712297850479185E-3,null,"*Prior to the 2011LTRA, the initial year of the 10-year assessment period is the report year (e.g., the 10-year assessment period for the 1990LTRA was 1990–1999). The 2011LTRA and subsequent LTRAs examine the initial year of the assessment period as one year out (e.g., the 10-year assessment period for the 2011LTRA is 2012–2023)."]
[2016,"2017–26",860286,918393,774436,826067.23912994482,58107,51631.239129944821,6.754381682370747E-2,6.6669471886566245E-2,7.288713354554277E-3,7.1970139133481492E-3]
[2017,"2018–27",863834.88823832804,912069.81219907396,764662.56813652802,806535.62040445395,48234.9239607458,41873.052267925799,5.5838129042361601E-2,5.47601700577156E-2,6.0554703063644402E-3,5.9412925621891198E-3]
[2018,"2019–28",855465.57563690585,900126.75809634128,766066.23993155418,807468.75127595884,44661.182459435426,41402.511344404658,5.2206872761869541E-2,5.4045602307319862E-2,5.6704321708249683E-3,5.8655481468439241E-3]
[2019,"2020-29",861156.15145410271,911372.76813325274,775462.51485488506,824208.0148917113,50216.616679150029,48745.500036826241,5.8313020924668432E-2,6.2859905028353508E-2,6.3172200704402215E-3,6.7966932370662203E-3]
[2020,"2021-30",860655.90541479271,905581.64850307943,776318.32782148954,825779.62232121429,44925.743088286719,49461.294499724754,5.2199424654658912E-2,6.3712645608307888E-2,5.6696412020782461E-3,6.8864124317580266E-3]
[2021,"2022-31",865343.07960237633,908768.07502330106,785865.15065294877,835893.22419930052,43424.995420924737,50028.073546351749,5.0182403308614253E-2,6.3659870277725281E-2,5.4552556248497197E-3,6.8808616495485975E-3]
[2022,"2023-32",872343.13125416136,925085.63486955164,787808.86765825062,850638.21996502788,52742.503615390277,62829.352306777262,6.046073124868051E-2,7.9752024743687533E-2,6.5439258410568968E-3,8.5621593949143371E-3]

{"sheet":"Table G","index":8,"n_rows":88,"n_cols":29,"rows_kept":88,"cut":false,"hidden":false,"merged":[[63,22,63,23],[63,24,63,25],[63,26,63,27],[64,26,64,27],[64,24,64,25],[64,22,64,23],[64,20,64,21],[64,18,64,19],[63,6,63,7],[63,8,63,9],[63,10,63,11],[63,12,63,13],[63,14,63,15],[63,16,63,17],[64,16,64,17],[64,14,64,15],[64,12,64,13],[64,10,64,11],[64,8,64,9],[64,6,64,7],[63,18,63,19],[63,20,63,21],[62,16,62,17],[62,18,62,19],[62,20,62,21],[62,22,62,23],[62,24,62,25],[62,26,62,27],[61,18,61,19],[61,20,61,21],[61,22,61,23],[61,24,61,25],[61,26,61,27],[61,16,61,17],[62,6,62,7],[62,8,62,9],[62,10,62,11],[62,12,62,13],[62,14,62,15],[61,6,61,7],[61,8,61,9],[61,10,61,11],[61,12,61,13],[61,14,61,15],[60,16,60,17],[60,18,60,19],[60,20,60,21],[60,22,60,23],[60,24,60,25],[60,26,60,27],[59,18,59,19],[59,20,59,21],[59,22,59,23],[59,24,59,25],[59,26,59,27],[59,16,59,17],[60,6,60,7],[60,8,60,9],[60,10,60,11],[60,12,60,13],[60,14,60,15],[59,6,59,7],[59,8,59,9],[59,10,59,11],[59,12,59,13],[59,14,59,15],[57,16,57,17],[57,18,57,19],[57,20,57,21],[57,22,57,23],[57,24,57,25],[57,26,57,27],[56,18,56,19],[56,20,56,21],[56,22,56,23],[56,24,56,25],[56,26,56,27],[56,16,56,17],[57,6,57,7],[57,8,57,9],[57,10,57,11],[57,12,57,13],[57,14,57,15],[56,6,56,7],[56,8,56,9],[56,10,56,11],[56,12,56,13],[56,14,56,15],[55,10,55,11],[55,12,55,13],[55,14,55,15],[53,20,53,21],[53,22,53,23],[53,24,53,25],[53,26,53,27],[54,6,54,7],[54,8,54,9],[54,10,54,11],[54,12,54,13],[54,14,54,15],[54,16,54,17],[55,16,55,17],[55,18,55,19],[55,20,55,21],[55,22,55,23],[55,24,55,25],[55,26,55,27],[54,18,54,19],[54,20,54,21],[54,22,54,23],[54,24,54,25],[54,26,54,27],[52,22,52,23],[52,24,52,25],[52,26,52,27],[53,6,53,7],[53,8,53,9],[53,10,53,11],[53,12,53,13],[53,14,53,15],[53,16,53,17],[53,18,53,19],[52,10,52,11],[52,12,52,13],[52,14,52,15],[52,16,52,17],[52,18,52,19],[52,20,52,21],[52,6,52,7],[52,8,52,9],[51,10,51,11],[51,12,51,13],[51,14,51,15],[49,20,49,21],[49,22,49,23],[49,24,49,25],[49,26,49,27],[50,6,50,7],[50,8,50,9],[50,10,50,11],[50,12,50,13],[50,14,50,15],[50,16,50,17],[51,16,51,17],[51,18,51,19],[51,20,51,21],[51,22,51,23],[51,24,51,25],[51,26,51,27],[50,18,50,19],[50,20,50,21],[50,22,50,23],[50,24,50,25],[50,26,50,27],[48,22,48,23],[48,24,48,25],[48,26,48,27],[49,6,49,7],[49,8,49,9],[49,10,49,11],[49,12,49,13],[49,14,49,15],[49,16,49,17],[49,18,49,19],[48,10,48,11],[48,12,48,13],[48,14,48,15],[48,16,48,17],[48,18,48,19],[48,20,48,21],[48,6,48,7],[48,8,48,9],[47,10,47,11],[47,12,47,13],[47,14,47,15],[45,20,45,21],[45,22,45,23],[45,24,45,25],[45,26,45,27],[46,6,46,7],[46,8,46,9],[46,10,46,11],[46,12,46,13],[46,14,46,15],[46,16,46,17],[47,16,47,17],[47,18,47,19],[47,20,47,21],[47,22,47,23],[47,24,47,25],[47,26,47,27],[46,18,46,19],[46,20,46,21],[46,22,46,23],[46,24,46,25],[46,26,46,27],[47,6,47,7],[47,8,47,9],[51,6,51,7],[51,8,51,9],[55,6,55,7],[55,8,55,9],[44,22,44,23],[44,24,44,25],[44,26,44,27],[45,6,45,7],[45,8,45,9],[45,10,45,11],[45,12,45,13],[45,14,45,15],[45,16,45,17],[45,18,45,19],[44,10,44,11],[44,12,44,13],[44,14,44,15],[44,16,44,17],[44,18,44,19],[44,20,44,21],[44,6,44,7],[44,8,44,9],[60,4,60,5],[61,4,61,5],[62,4,62,5],[63,4,63,5],[56,4,56,5],[57,4,57,5],[59,4,59,5],[64,4,64,5],[53,4,53,5],[54,4,54,5],[55,4,55,5],[44,4,44,5],[45,4,45,5],[46,4,46,5],[47,4,47,5],[48,4,48,5],[49,4,49,5],[50,4,50,5],[51,4,51,5],[52,4,52,5],[58,16,58,17],[58,18,58,19],[58,20,58,21],[58,22,58,23],[58,24,58,25],[58,26,58,27],[58,4,58,5],[58,6,58,7],[58,8,58,9],[58,10,58,11],[58,12,58,13],[58,14,58,15],[43,16,43,17],[43,18,43,19],[43,20,43,21],[43,22,43,23],[43,24,43,25],[43,26,43,27],[43,4,43,5],[43,6,43,7],[43,8,43,9],[43,10,43,11],[43,12,43,13],[43,14,43,15]]}
[]
[]
[]
[null,"9-Year Growth; *10-Year Growth","9-Year Growth; *10-Year Growth","CAGR %"]
[1990,613039,613.03899999999999,2.0853606637524669E-2]
[1991,582979,582.97900000000004,1.9502348181675844E-2]
[1992,580494,580.49400000000003,1.9126471565118708E-2]
[1993,565933,565.93299999999999,1.8456799405107471E-2]
[1994,551791,551.79100000000005,1.7780765072508142E-2]
[1995,583140,583.14,1.8258895027518429E-2]
[1996,545376,545.37599999999998,1.6643497748993763E-2]
[1997,568679,568.67899999999997,1.7030944675862525E-2]
[1998,554829,554.82899999999995,1.6311287618437698E-2]
[1999,636545,636.54499999999996,1.8166892748121555E-2]
[2000,628889,628.88900000000001,1.749501455086766E-2]
[2001,697677,697.67700000000002,1.8737986355379155E-2]
[2002,654751,654.75099999999998,1.7768965310961837E-2]
[2003,684444,684.44399999999996,1.810368438318144E-2]
[2004,630818,630.81799999999998,1.6712668541647657E-2]
[2005,678259,678.25900000000001,1.759516457601551E-2]
[2006,666689,666.68899999999996,1.7185435380447034E-2]
[2007,657408,657.40800000000002,1.6625278403162858E-2]
[2008,620306.79,620.30679000000009,1.5598577798215496E-2]
[2009,589356,589.35599999999999,1.508170792616359E-2]
[2010,711734,711.73400000000004,1.8488129320549662E-2]
["2011*",568323.46917677112,568.32346917677114,1.2981329496820404E-2]
[2012,485299.74701994285,485.29974701994286,1.1110775937205775E-2]
[2013,546873,546.87300000000005,1.2454961739159387E-2]
[2014,441886,441.88600000000002,1.0103806679322647E-2]
[2015,372824,372.82400000000001,8.5162311795756729E-3]
[2016,303884,303.88400000000001,7.0935153822750951E-3]
[2017,261392,261.392,6.0789472892543994E-3]
[2018,249299.79999999981,249.29979999999981,5.8703390515375542E-3]
[2019,255708.83181331772,255.70883181331772,6.0000000000000053E-3]
[2020,181756.40810068045,181.75640810068046,4.3252323671683079E-3]
[2021,276748.18483710103,276.74818483710101,6.4808573406758274E-3]
[2021,296988.14013795648,296.98814013795646,6.7042832504651262E-3]
[]
[]
[]
[]
[]
[]
[null,"NET ENERGY FOR LOAD (NEL)- MONTHLY","Year(s)","Unit","JAN (W)",null,"FEB (W)",null,"MAR",null,"APR",null,"MAY",null,"JUN (S)",null,"JUL (S)",null,"AUG (S)",null,"SEP (S)",null,"OCT",null,"NOV",null,"DEC (W)",null,"Year Total"]
["MISO","Net Energy For Load - Year 1 Forecast",2023,"GWh",59758.299999999974,null,52905.000000000007,null,53567.099999999984,null,49287.3,null,53044.700000000019,null,58858.19999999999,null,65706.39999999998,null,64230.200000000019,null,59729.900000000009,null,52522,null,52277.799999999996,null,57890.499999999993,null,679777.4]
["MRO-Manitoba","Net Energy For Load - Year 1 Forecast",2023,"GWh",2792.7564383582499,null,2449.8566754490198,null,2369.5824017387399,null,1911.26540457391,null,1728.5744650611,null,1635.52876654324,null,1822.6959422995201,null,1762.9726011263299,null,1661.20827526618,null,1953.13253579722,null,2260.9210107333502,null,2654.5214234882701,null,25003.015940435129]
["MRO-SaskPower","Net Energy For Load - Year 1 Forecast",2023,"GWh",2453.6999999999998,null,2156,null,2267.6999999999998,null,2091.4,null,2044.7,null,1977.6,null,2101.4,null,2104.1999999999998,null,1954.8,null,2176.4,null,2255.1999999999998,null,2406.6999999999998,null,25989.800000000003]
["NPCC-Maritimes","Net Energy For Load - Year 1 Forecast",2023,"GWh",3108.028283517981,null,2793.9941472562973,null,2742.1252645019104,null,2273.5228079739304,null,2061.7411918918001,null,1858.5241390928832,null,1973.8841939915515,null,1990.7784851777401,null,1878.190658986259,null,2101.5400941375456,null,2376.8939265569052,null,2859.9065920728226,null,28019.129785157624]
["NPCC-New England","Net Energy For Load - Year 1 Forecast",2023,"GWh",11412,null,10083,null,10254,null,9094,null,9269,null,10353,null,12385,null,11925,null,9870,null,9618,null,9821,null,11152,null,125236]
["NPCC-New York","Net Energy For Load - Year 1 Forecast",2023,"GWh",13351.191409339623,null,11812.125125973538,null,12187.010701399324,null,10811.462063320489,null,11356.009593760014,null,13090.671427735146,null,15588.095989896538,null,15217.344502956099,null,12598.983587069461,null,11607.082333375358,null,11662.179889693934,null,12837.843375480472,null,152120]
["NPCC-Ontario","Net Energy For Load - Year 1 Forecast",2023,"GWh",13086.07488646718,null,11629.512701499902,null,11983.155429268518,null,10426.159745393184,null,10494.585290660778,null,11174.791791608852,null,12232.79362632869,null,12182.574692268769,null,10778.945919495109,null,10971.219044289617,null,11442.211385649294,null,12346.763678661689,null,138748.78819159156]
["NPCC-Quebec","Net Energy For Load - Year 1 Forecast",2023,"GWh",22765.810147774402,null,20421.7646273596,null,19141.019306900402,null,15641.845997411699,null,13699.554368085901,null,13008.551916560198,null,13763.5031818389,null,13624.966098647999,null,12847.594016744601,null,14546.445940274099,null,17126.585074088202,null,21075.7828998039,null,197663.4235754899]
["PJM","Net Energy For Load - Year 1 Forecast",2023,"GWh",75404,null,65386,null,65717,null,55483,null,58728,null,65543,null,75361,null,73084,null,61215,null,58375,null,61997,null,71468,null,787761]
["SERC-C","Net Energy For Load - Year 1 Forecast",2023,"GWh",20813,null,18004,null,17093,null,15200,null,16614,null,19077,null,20994,null,20860,null,17424,null,15942,null,16390,null,19035,null,217446]
["SERC-E","Net Energy For Load - Year 1 Forecast",2023,"GWh",21701,null,19347,null,17903,null,16722,null,18208,null,21197,null,23358,null,22707,null,19383,null,16754,null,18323,null,20480,null,236083]
["SERC-FP","Net Energy For Load - Year 1 Forecast",2023,"GWh",19237,null,17179,null,18594,null,19324,null,22417,null,24123,null,25773,null,25839,null,23812,null,21732,null,18331,null,19037,null,255398]
["SERC-SE","Net Energy For Load - Year 1 Forecast",2023,"GWh",21304,null,17901,null,17656,null,16784,null,19611,null,21979,null,24231,null,23715,null,20072,null,17854,null,17643,null,20229,null,238979]
["SPP","Net Energy For Load - Year 1 Forecast",2023,"GWh",24985.5,null,22119.4,null,22065.3,null,20142.3,null,21774.2,null,25272.9,null,28752,null,28391.200000000001,null,23793.5,null,21801.5,null,21817.8,null,24290.1,null,285205.7]
["Texas RE-ERCOT","Net Energy For Load - Year 1 Forecast",2023,"GWh",35119.339686066662,null,30833.806459266671,null,32437.143014866673,null,32313.612920133335,null,37009.360968866677,null,41032.761947599989,null,44096.696923266667,null,45046.141371866674,null,38935.418661266667,null,35366.709108733332,null,32257.229279733336,null,35236.119071466659,null,439684.33941313333]
["WECC-AB","Net Energy For Load - Year 1 Forecast",2023,"GWh",7881.9261189999997,null,7126.8485360000004,null,7695.2381939999996,null,6795.6987939999999,null,6913.0169150000002,null,6748.4996709999996,null,7263.2907089999999,null,7338.7923600000004,null,6813.9799499999999,null,7172.2456940000002,null,7456.1557579999999,null,7812.0556260000003,null,87017.748326000001]
["WECC-BC","Net Energy For Load - Year 1 Forecast",2023,"GWh",6372.9467741050885,null,7126.8485360000004,null,7695.2381939999996,null,6795.6987939999999,null,6913.0169150000002,null,6748.4996709999996,null,7263.2907089999999,null,7338.7923600000004,null,6813.9799499999999,null,7172.2456940000002,null,7456.1557579999999,null,7812.0556260000003,null,85508.76898110508]
["WECC-CA/MX","Net Energy For Load - Year 1 Forecast",2023,"GWh",21041.378920673829,null,18464.876774401488,null,20140.251720171571,null,19516.623533974751,null,21126.933696394553,null,23533.365744289309,null,26708.80412055898,null,27302.83644706232,null,25058.707479060835,null,22133.659969391618,null,19954.258928412233,null,21404.632153447634,null,266386.32948783913]
["WECC-WPP","Net Energy For Load - Year 1 Forecast",2023,"GWh",35609.087418646232,null,31870.577003061273,null,32248.946991914483,null,29813.506133022493,null,30858.8794179793,null,34127.799830557051,null,38183.046177826058,null,36972.969315337301,null,32432.200553911131,null,30971.558650464507,null,31808.27284155881,null,36236.274113168125,null,401133.11844744679]
["WECC-SRSG","Net Energy For Load - Year 1 Forecast",2023,"GWh",8713.2036257118671,null,7512.213906157308,null,7959.5282866467896,null,8270.7524720730598,null,9740.2562648635358,null,11876.000591267668,null,13455.973063949679,null,13235.160274851922,null,11404.334936791023,null,9300.5615983920288,null,8049.3426812074122,null,8827.0963213404684,null,118344.42402325277]
["Total",null,null,null,426910.24370966107,null,377122.82449242508,null,381716.33950540842,null,348698.14866587688,null,373612.52908756363,null,413215.69549725432,null,461013.87463795661,null,454868.92850929522,null,398477.74398859136,null,370071.30066285527,null,370706.00653363334,null,415091.35088093003,null,4791504.9861714514]
[]
[null,"NET ENERGY FOR LOAD(NEL)  - ANNUAL","Year(s)","Unit",2032]
["MISO","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",653654.76071428601]
["MRO-Manitoba","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",26800.233131299901]
["MRO-SaskPower","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",28474.3]
["NPCC-Maritimes","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",28288.752550840254]
["NPCC-New England","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",143826]
["NPCC-New York","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",154520]
["NPCC-Ontario","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",160081.23883677309]
["NPCC-Quebec","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",210931.93850293552]
["PJM","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",845133]
["SERC-C","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",223646]
["SERC-E","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",248593]
["SERC-FP","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",278034]
["SERC-SE","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",240816]
["SPP","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",307219.75599999999]
["Texas RE-ERCOT","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",508445.330908]
["WECC-AB","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",92732.527960000007]
["WECC-BC","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",71346.844957722788]
["WECC-CA/MX","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",295368.17901087762]
["WECC-WPP","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",431721.0608595807]
["WECC-SRSG","Net Energy for Load - Year 2-10 Forecast","2024-2032","GWh",136828.20287709226]
["Total",null,null,null,5088493.1263094079]

{"sheet":"Table H","index":9,"n_rows":76,"n_cols":17,"rows_kept":76,"cut":false,"hidden":false,"merged":[[30,14,30,15],[54,14,54,15]]}
[]
[]
[]
[]
[]
["NERC-Wide Peak Total Internal Demand Demand Growth",null,null,null,null,null,null,null,null,null,null,null,null,null,"Period","Years"]
[null,"Peak Season",2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,"CAGR %",null,9,1]
["WECC-SRSG","S",27038.891873796656,27154.149535318989,27863.55633027968,28516.318143813842,29185.664862307221,29633.895956429165,30048.73699671018,30512.678138707801,30935.473157171968,31440.91628039939,1.6900540905521177E-2,null,null,null,"Figure 29"]
["NPCC-Ontario","S",22930.472903693513,23489.659460130013,23855.683323612448,24104.44495781789,24288.290635793081,24477.05411664745,25166.216052499673,25081.43619709009,25678.173929375589,25693.565235509843,1.2721782055282738E-2]
["WECC-CA/MX","S",57090.970320091968,57759.300586376434,58609.038029210285,59184.34834367624,60027.845771859145,60652.245445320397,61423.295019860539,62163.522176017679,62967.318898467369,63526.125029053597,1.1937947763494883E-2]
["MRO-Manitoba Hydro","W",4622,4628.1940270077766,4638.3253957043944,4650.0577646877928,4843.6130442953945,4861.7846334484393,4894.1995947756559,4945.1264509215953,5008.163775580636,5080.4192258635694,1.0562759652664733E-2]
["MRO-SaskPower","W",3804,3827,3916,3940,3999,4056,4101,4128,4156,4178,1.0474423187382786E-2]
["Texas RE-ERCOT","S",79328.625352133327,80553.618545066667,81581.340911333347,82605.758452533337,83398.064937733332,84146.103560599993,84878.12974293335,85569.332573199979,86233.212782133342,86863.385693999997,1.0132945900049428E-2]
["WECC-WPP","S",67257.979962626167,68558.542352960823,69474.50015359484,69635.514523244361,70388.537856700379,71095.243123094595,71714.883341036853,72228.593967390698,72827.473679900912,73612.950319962489,1.0082185406917299E-2]
["WECC-BC","W",11551.513241670855,11571.828637652587,11711.35830178359,11849.791633724837,11991.533955352792,12121.648993625216,12235.620533639472,12357.014625179385,12483.108858131691,12634.541128203937,1.0007294471555683E-2]
["SERC-FP","S",52427,52857,53140,53654,54128,54605,55322,56010,56600,57313,9.9498121701417919E-3]
["SPP","S",52397.93,52999.15,53383.24,53997.55,54219.68,54451.61,54697.11,55640.77,55872.77,56160.74,7.7354148729229522E-3]
["NPCC-Québec","W",40183.10109694054,40557.933534718941,40865.157368751235,41200.324570433142,41542.735166313338,41920.565109163741,42188.101494722541,42430.872740454637,42645.013261995242,42962.039161653636,7.4577133724043065E-3]
["NPCC-Maritimes","W",5636.2432996315147,5726.8416669300086,5750.2078848476613,5771.9153931515903,5805.169337052087,5839.5130006823201,5862.4177192850148,5905.1836046120343,5944.8998736011163,5993.7884022577155,6.8573944057612746E-3]
["SERC-E","W",44878,44996,45091,45320,45490,45953,46135,46706,47164,47636,6.6487925075122689E-3]
["WECC-AB","W",11961.120779999999,11961.120779999999,12064.83793,12154.34411,12256.874970000001,12373.244140000001,12362.08287,12413.36967,12547.872310000001,12621.94327,5.9929276980297264E-3]
["NPCC-New England","S",24633,24600,24579,24592,24631,24722,24869,25071,25322,25576,4.1828799637488867E-3]
["PJM","S",149351,150309,151165,152259,152322,152689,153334,153775,154275,154381,3.6872627000414937E-3]
["MISO","S",124950.089318358,126090.83045564751,126211.5763572517,126297.8096962158,126630.8222783472,126964.9884837423,127239.9353615991,127652.4518136562,128319.7267364547,128317.11735050099,2.9588473526500625E-3]
["SERC-C","W",42119,42080,42128,42190,42328,42403,42509,42606,42793,42848,1.9084882070652398E-3]
["NPCC-New York","S",32018,31778,31505,31339,31292,31317,31468,31684,31946,32214,6.7832951843449507E-4]
["SERC-SE","S",46082,45630,45826,45814,46022,44638,44826,44938,45290,45586,-1.2016958719477389E-3]
["TOTAL","-",245169.08931835799,245578.83045564749,245670.5763572517,245640.80969621579,246272.82227834722,245322.98848374229,246042.93536159908,246880.4518136562,248348.7267364547,248965.11735050101,1.7086428153372246E-3]
[]
["NERC-Wide Summer Total Internal Demand Demand Growth"]
[null,"Summer",2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,"CAGR %",null," Top 5 Summer Demand Change"]
["WECC-SRSG","S",27038.891873796656,27154.149535318989,27863.55633027968,28516.318143813842,29185.664862307221,29633.895956429165,30048.73699671018,30512.678138707801,30935.473157171968,31440.91628039939,1.6900540905521177E-2,null,"Assessment Area","Demand Change"]
["NPCC-Ontario","S",22930.472903693513,23489.659460130013,23855.683323612448,24104.44495781789,24288.290635793081,24477.05411664745,25166.216052499673,25081.43619709009,25678.173929375589,25693.565235509843,1.2721782055282738E-2,null,"WECC-SRSG",1.6900540905521177E-2]
["WECC-CA/MX","S",57090.970320091968,57759.300586376434,58609.038029210285,59184.34834367624,60027.845771859145,60652.245445320397,61423.295019860539,62163.522176017679,62967.318898467369,63526.125029053597,1.1937947763494883E-2,null,"NPCC-Ontario",1.2721782055282738E-2]
["MRO-SaskPower","S",3521,3543,3626,3648,3703,3755,3797,3822,3848,3868,1.0498340161281039E-2,null,"WECC-CA/MX",1.1937947763494883E-2]
["NPCC-Maritimes","S",3361.5382982339088,3499.9349916286146,3518.4978321355275,3547.9035787590642,3566.4134534065111,3584.3886919325664,3602.8749102630231,3629.0725981550177,3655.041182108524,3686.0506478387661,1.0292260640648809E-2,null,"MRO-SaskPower",1.0498340161281039E-2]
["Texas RE-ERCOT","S",79328.625352133327,80553.618545066667,81581.340911333347,82605.758452533337,83398.064937733332,84146.103560599993,84878.12974293335,85569.332573199979,86233.212782133342,86863.385693999997,1.0132945900049428E-2,null,"NPCC-Maritimes",1.0292260640648809E-2]
["WECC-WPP","S",67257.979962626167,68558.542352960823,69474.50015359484,69635.514523244361,70388.537856700379,71095.243123094595,71714.883341036853,72228.593967390698,72827.473679900912,73612.950319962489,1.0082185406917299E-2]
["SERC-FP","S",52427,52857,53140,53654,54128,54605,55322,56010,56600,57313,9.9498121701417919E-3]
["WECC-BC","S",8568.5641450472103,8568.5641450472103,8671.1148944172801,8772.4432384165284,8877.1862579443259,8973.7468256709071,9058.7839536992051,9149.3944504452156,9243.6126251551796,9356.5819859154581,9.8234785864881324E-3]
["SPP","S",52397.93,52999.15,53383.24,53997.55,54219.68,54451.61,54697.11,55640.77,55872.77,56160.74,7.7354148729229522E-3]
["SERC-E","S",43123,43372,43549,43761,44070,44265,44654,45092,45607,46111,7.4716675102759478E-3]
["WECC-AB","S",11206.054480000001,11233.333049999999,11421.709489999999,11510.092640000001,11733.77432,11525.24181,11673.15605,11634.91804,11819.09727,11839.070599999999,6.1243351813100588E-3]
["NPCC-Québec","S",22656.014600180697,22717.731750900399,22891.092030477299,23053.304173440098,23210.043572008599,23399.913555120198,23568.4065603862,23666.6375347627,23764.803455379999,23871.9667007715,5.8257336519560443E-3]
["MRO-Manitoba Hydro","S",3058,3050.3948310704591,2969.9470407437916,2973.8326057647246,3132.3155501119413,3131.5192879165606,3144.5583178543234,3138.089028125642,3169.8334437189806,3216.1650255996733,5.6189000696578173E-3]
["NPCC-New England","S",24633,24600,24579,24592,24631,24722,24869,25071,25322,25576,4.1828799637488867E-3]
["PJM","S",149351,150309,151165,152259,152322,152689,153334,153775,154275,154381,3.6872627000414937E-3]
["MISO","S",124950.089318358,126090.83045564751,126211.5763572517,126297.8096962158,126630.8222783472,126964.9884837423,127239.9353615991,127652.4518136562,128319.7267364547,128317.11735050099,2.9588473526500625E-3]
["SERC-C","S",41343,41791,41787,41794,41825,41978,42052,42145,42235,42452,2.9455413111407758E-3]
["NPCC-New York","S",32018,31778,31505,31339,31292,31317,31468,31684,31946,32214,6.7832951843449507E-4]
["SERC-SE","S",46082,45630,45826,45814,46022,44638,44826,44938,45290,45586,-1.2016958719477389E-3]
["TOTAL","S",872343.13125416136,879555.20970414719,885628.29639305617,891060.3203536818,896651.63949621178,900004.950856474,906538.08630684239,912603.89651755104,919609.53715986665,925085.63486955164,6.5439258410568968E-3]
[]
["NERC-Wide Winter Total Internal Demand Demand Growth"]
[null,"Peak Season",2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,"CAGR %",null,"Top 5 Winter Demand Change"]
["NPCC-New York","W",24287,24481,24735,25098,25575,26171,26884,27719,28756,29954,2.3576027121603005E-2,null,"Assessment Area","Demand Change"]
["WECC-SRSG","W",16587.943761246817,16199.900209173178,16896.047118370996,17446.646026843813,18033.618985899979,18497.099905509149,18926.464173753408,19294.498193537569,19637.278291231272,19928.801503080238,2.0597010578122354E-2,null,"NPCC-New York",2.3576027121603005E-2]
["NPCC-New England","W",20090,20223,20405,20607,20881,21236,21678,22226,22852,23496,1.7553168031725574E-2,null,"WECC-SRSG",2.0597010578122354E-2]
["NPCC-Ontario","W",22041.961635571111,22277.240361910364,22819.605484372198,22915.645487926522,23279.686173758659,23933.082611074577,24056.132187792002,24315.958884906162,24542.39786464331,24793.784249102056,1.315747470201023E-2,null,"NPCC-New England",1.9461870520303348E-2]
["Texas RE-ERCOT","W",66454.289111533304,67699.428096866657,68858.012803733334,69793.082537266673,70697.449819200003,71558.416991266669,72391.611367266654,73178.310706200005,73931.185242466672,74660.404174133335,1.3021332887786397E-2,null,"NPCC-Ontario",1.315747470201023E-2]
["WECC-CA/MX","W",39585.100710424318,39585.100710424318,40153.376836825344,40655.223301972379,41207.292471870511,41795.589321816122,42229.266095680192,42933.931746086273,43406.841233022235,44017.042487491148,1.1861359607979516E-2,null,"Texas RE-ERCOT",1.3021332887786397E-2]
["MRO-Manitoba Hydro","W",4622,4628.1940270077766,4638.3253957043944,4650.0577646877928,4843.6130442953945,4861.7846334484393,4894.1995947756559,4945.1264509215953,5008.163775580636,5080.4192258635694,1.0562759652664733E-2]
["MRO-SaskPower","W",3804,3827,3916,3940,3999,4056,4101,4128,4156,4178,1.0474423187382786E-2]
["WECC-BC","W",11551.513241670855,11571.828637652587,11711.35830178359,11849.791633724837,11991.533955352792,12121.648993625216,12235.620533639472,12357.014625179385,12483.108858131691,12634.541128203937,1.0007294471555683E-2]
["WECC-WPP","W",59505.60843916607,60540.840492080533,61290.556859044154,61474.879420457706,62075.562142311406,62568.606888110968,63159.394529106969,63639.892311242183,64251.962257720312,64944.362305117109,9.7651903521616124E-3]
["SPP","W",42174.29,42569.09,43200.35,43557.03,43640.480000000003,43945.69,44938.51,45204.69,45475.11,45746.11,9.0738048570533358E-3]
["SERC-FP","W",49014,49239,49764,50246,50127,50684,51228,51773,52420,53008,8.742087906183249E-3]
["NPCC-Québec","W",40183.10109694054,40557.933534718941,40865.157368751235,41200.324570433142,41542.735166313338,41920.565109163741,42188.101494722541,42430.872740454637,42645.013261995242,42962.039161653636,7.4577133724043065E-3]
["NPCC-Maritimes","W",5636.2432996315147,5726.8416669300086,5750.2078848476613,5771.9153931515903,5805.169337052087,5839.5130006823201,5862.4177192850148,5905.1836046120343,5944.8998736011163,5993.7884022577155,6.8573944057612746E-3]
["SERC-E","W",44878,44996,45091,45320,45490,45953,46135,46706,47164,47636,6.6487925075122689E-3]
["PJM","W",134360,135521,136923,137943,138809,139318,140109,140682,141516,142314,6.4108084062866055E-3]
["WECC-AB","W",11961.120779999999,11961.120779999999,12064.83793,12154.34411,12256.874970000001,12373.244140000001,12362.08287,12413.36967,12547.872310000001,12621.94327,5.9929276980297264E-3]
["MISO","W",102502.6955820662,105147.90565817359,105123.34309618321,105281.149145135,105707.65327926481,105994.7132013908,106410.16177924319,106878.14828323149,107211.4012035429,107409.984058125,5.2095273764518613E-3]
["SERC-C","W",42119,42080,42128,42190,42328,42403,42509,42606,42793,42848,1.9084882070652398E-3]
["SERC-SE","W",46451,45288,45474,45733,44877,45161,45376,45719,46034,46411,-9.5716913520393909E-5]
["TOTAL","W",787808.86765825062,794120.424174938,801807.17907961621,807827.08939159929,813167.66934531892,820391.95479608804,827673.96234526508,835055.99721637147,842776.23417193536,850638.21996502788,8.5621593949143371E-3]

{"sheet":"Table I","index":10,"n_rows":76,"n_cols":40,"rows_kept":76,"cut":false,"hidden":false,"merged":[[2,28,2,39],[21,28,21,39],[40,28,40,39],[59,28,59,39],[21,0,21,11],[40,0,40,11],[59,0,59,11],[21,14,21,25],[40,14,40,25],[59,14,59,25],[2,14,2,25],[2,0,2,11]]}
[null,null,null,null,null,null,"See Demand Assumptions and Resource Categories description in the 2022 LTRA for definitions of generating unit status tiers"]
[]
["Existing - Eastern",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Eastern",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Eastern"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",165850.264,161672.96399999998,157502.764,155410.264,154316.76400000002,150151.16399999999,145788.56400000001,141227.86400000009,138945.76400000008,138945.76400000008,136930.76400000008,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",165850.264,161672.96399999998,157502.764,155410.264,154316.76400000002,150151.16399999999,145788.56400000001,141227.86400000009,138945.76400000008,138945.76400000008,136930.76400000008]
["Petroleum",32969.172000000071,32190.325000000026,32200.989000000027,32037.017000000025,31866.017000000025,31675.917000000027,31675.917000000027,31675.917000000027,31502.317000000025,31448.617000000024,31448.617000000024,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",32969.172000000071,32190.325000000026,32200.989000000027,32037.017000000025,31866.017000000025,31675.917000000027,31675.917000000027,31675.917000000027,31502.317000000025,31448.617000000024,31448.617000000024]
["Natural Gas and Other Gases",330214.91066666727,329942.41066666716,328800.47666666715,326068.18066666741,324600.80066666723,321679.30066666723,319985.30066666723,319982.50066666724,319829.60066666722,318618.10066666728,318618.10066666728,null,null,"Natural Gas and Other Gases",1930.4489994049072,10259.204187788298,15936.14330350504,17945.343303505033,19027.54330350503,20899.54330350503,23646.54330350503,27150.543303505016,27569.543303505016,27988.543303505016,30286.543303505008,null,null,"Natural Gas and Other Gases",332145.35966607218,340201.61485445546,344736.61997017218,344013.52397017245,343628.34397017228,342578.84397017228,343631.84397017228,347133.04397017224,347399.14397017221,346606.64397017227,348904.64397017227]
["Biomass",4100.0479999999989,4097.9030000000012,4045.3950000000032,3978.5850000000032,3978.5850000000032,3872.6850000000027,3841.1850000000027,3841.1850000000027,3808.1850000000027,3808.1850000000027,3808.1850000000027,null,null,"Biomass",0,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,56.400000000000006,null,null,"Biomass",4100.0479999999989,4154.3030000000008,4101.7950000000028,4034.9850000000033,4034.9850000000033,3929.0850000000028,3897.5850000000028,3897.5850000000028,3864.5850000000028,3864.5850000000028,3864.5850000000028]
["Solar",11717.021300000004,11656.1113,11714.011299999996,11690.211299999997,11669.811300000003,11665.6113,11661.511299999996,11659.311300000001,11655.211300000001,11650.1113,11649.4113,null,null,"Solar",401.93,13589.128500000001,21958.79049949647,22860.630499496467,23246.530499496472,23444.280499496472,23681.070499496473,23913.090499496469,24012.800499496472,24117.390499496472,24158.990499496475,null,null,"Solar",12118.951300000004,25245.239800000003,33672.801799496468,34550.841799496462,34916.341799496477,35109.891799496472,35342.581799496467,35572.401799496467,35668.011799496475,35767.501799496473,35808.401799496474]
["Wind",14542.965046072009,14323.615046072011,14322.715046072009,14316.115046072011,14300.966659106096,14290.366659106096,14239.606659106097,14225.706659106098,14213.506659106097,14207.706659106098,14205.706659106098,null,null,"Wind",2700,5056.0425599999999,6231.8405599999996,10178.572560000001,10662.072560000001,10929.572560000001,10929.572560000001,10929.572560000001,10929.572560000001,10929.572560000001,10929.572560000001,null,null,"Wind",17242.965046072008,19379.657606072011,20554.555606072008,24494.68760607201,24963.039219106096,25219.939219106098,25169.179219106096,25155.279219106098,25143.079219106097,25137.279219106098,25135.279219106098]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",35647.46400810175,35279.852433101769,35277.152433101772,35277.152433101772,35277.152433101772,35277.152433101772,35277.152433101772,35258.742340536293,35258.742340536293,35123.342340536285,35126.44234053629,null,null,"Conventional Hydro",206.00000000000003,371.98552628998522,381.48552628998522,393.48552628998522,393.48552628998522,455.48552628998533,455.48552628998533,451.88300314861613,451.88300314861613,451.88300314861613,451.88300314861613,null,null,"Conventional Hydro",35853.46400810175,35651.837959391756,35658.637959391759,35670.637959391759,35670.637959391759,35732.637959391759,35732.637959391759,35710.625343684907,35710.625343684907,35575.225343684899,35578.325343684905]
["Run of River Hydro",1599.1480000000026,1599.1480000000026,1599.1480000000026,1599.1480000000026,1599.1480000000026,1489.1480000000006,1489.1480000000006,1489.1480000000006,1489.1480000000006,1489.1480000000006,1489.1480000000006,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",1599.1480000000026,1599.1480000000026,1599.1480000000026,1599.1480000000026,1599.1480000000026,1489.1480000000006,1489.1480000000006,1489.1480000000006,1489.1480000000006,1489.1480000000006,1489.1480000000006]
["Pumped Storage",18268.684799999999,18284.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,18304.984799999998,null,null,"Pumped Storage",66,66,66,66,66,66,66,66,66,66,66,null,null,"Pumped Storage",18334.684799999999,18350.984799999998,18370.984799999998,18370.984799999998,18370.984799999998,18370.984799999998,18370.984799999998,18370.984799999998,18370.984799999998,18370.984799999998,18370.984799999998]
["Nuclear",93409.108000000022,91786.108000000022,93481.850802665576,92556.850802665591,92564.850802665591,91338.850802665591,91291.850802665591,91291.850802665591,92109.850802665591,91352.850802665591,91352.850802665591,null,null,"Nuclear",0,2200,2200,2200,2200,2200,2200,2200,2200,2200,2200,null,null,"Nuclear",93409.108000000022,93986.108000000022,95681.850802665576,94756.850802665591,94764.850802665591,93538.850802665591,93491.850802665591,93491.850802665591,94309.850802665591,93552.850802665591,93552.850802665591]
["Hybrid",29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,29.520000000000007,null,null,"Hybrid",0,1249.5400000000002,1333.3482000000004,1333.3482000000004,1333.3482000000004,1333.3482000000004,1333.3482000000004,1333.3482000000004,1333.3482000000004,1333.3482000000004,1333.3482000000004,null,null,"Hybrid",29.520000000000007,1279.0600000000002,1362.8682000000003,1362.8682000000003,1362.8682000000003,1362.8682000000003,1362.8682000000003,1362.8682000000003,1362.8682000000003,1362.8682000000003,1362.8682000000003]
["Other",2881.5030000000006,2885.2530000000006,2885.1530000000007,2862.1530000000007,2847.4530000000004,2843.5530000000008,2843.5530000000008,2831.8530000000001,2831.8530000000001,2831.8530000000001,2831.8530000000001,null,null,"Other",0,695,755,755,755,755,755,755,755,755,755,null,null,"Other",2881.5030000000006,3580.2530000000006,3640.1530000000007,3617.1530000000007,3602.4530000000004,3598.5530000000008,3598.5530000000008,3586.8530000000001,3586.8530000000001,3586.8530000000001,3586.8530000000001]
["Battery",555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,555.34500000000003,null,null,"Battery",8.3000000000000007,86.6,692.2,713.32,713.32,1063.32,1423.32,2110.3200000000002,2482.3200000000002,3032.32,3032.32,null,null,"Battery",563.64499999999998,641.94500000000005,1247.5450000000001,1268.665,1268.665,1618.665,1978.665,2665.665,3037.665,3587.665,3587.665]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing - Quebec",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Quebec",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Quebec"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0]
["Petroleum",436,436,436,436,436,436,436,436,436,436,436,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",436,436,436,436,436,436,436,436,436,436,436]
["Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0,null,null,"Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0,null,null,"Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0]
["Biomass",403.68200000000002,395.58199999999999,395.58199999999999,395.58199999999999,395.58199999999999,285.78199999999998,218.232,218.232,218.232,218.232,210.63200000000001,null,null,"Biomass",9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,null,null,"Biomass",413.18200000000002,405.08199999999999,405.08199999999999,405.08199999999999,405.08199999999999,295.28199999999998,227.732,227.732,227.732,227.732,220.13200000000001]
["Solar",0,0,0,0,0,0,0,0,0,0,0,null,null,"Solar",0,0,0,0,0,0,0,0,0,0,0,null,null,"Solar",0,0,0,0,0,0,0,0,0,0,0]
["Wind",1375.2540000000004,1375.2540000000004,1375.2540000000004,1356.4620000000004,1298.2500000000005,1262.0700000000004,1222.6500000000003,1174.6620000000003,1174.6620000000003,1117.4220000000003,872.15399999999988,null,null,"Wind",0,0,73.44,73.44,73.44,73.44,73.44,73.44,73.44,73.44,73.44,null,null,"Wind",1375.2540000000004,1375.2540000000004,1448.6940000000004,1429.9020000000005,1371.6900000000005,1335.5100000000004,1296.0900000000004,1248.1020000000003,1248.1020000000003,1190.8620000000003,945.59399999999982]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",39794.693499999994,39803.336357142849,39808.979214285704,39814.622071428559,39820.264928571429,39822.907785714284,39825.550642857139,39828.193499999994,39830.836357142849,39833.479214285704,39836.122071428559,null,null,"Conventional Hydro",245,245,245,245,245,245,245,245,245,245,245,null,null,"Conventional Hydro",40039.693499999994,40048.336357142849,40053.979214285704,40059.622071428559,40065.264928571429,40067.907785714284,40070.550642857139,40073.193499999994,40075.836357142849,40078.479214285704,40081.122071428559]
["Run of River Hydro",103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,93.518000000000001,80.2,55.2,null,null,"Run of River Hydro",0,0,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,null,null,"Run of River Hydro",103.41800000000001,103.41800000000001,144.11799999999999,144.11799999999999,144.11799999999999,144.11799999999999,144.11799999999999,144.11799999999999,134.21800000000002,120.9,95.9]
["Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0]
["Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0]
["Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hybrid",0,0,0,0,0,0,0,0,0,0,0]
["Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0]
["Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing - Texas",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Texas",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Texas"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",12957.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",12957.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6,13567.6]
["Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0]
["Natural Gas and Other Gases",48211.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,48350.600000000013,null,null,"Natural Gas and Other Gases",0,492.8,503.8,503.8,503.8,503.8,503.8,503.8,503.8,503.8,503.8,null,null,"Natural Gas and Other Gases",48211.600000000013,48843.400000000016,48854.400000000016,48854.400000000016,48854.400000000016,48854.400000000016,48854.400000000016,48854.400000000016,48854.400000000016,48854.400000000016,48854.400000000016]
["Biomass",162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,null,null,"Biomass",0,0,0,0,0,0,0,0,0,0,0,null,null,"Biomass",162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998,162.79999999999998]
["Solar",9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,9383.1210000000028,null,null,"Solar",0,9402.4719000000005,20383.309800000003,22319.452799999999,22481.452799999999,22481.452799999999,22481.452799999999,22481.452799999999,22481.452799999999,22481.452799999999,22481.452799999999,null,null,"Solar",9383.1210000000028,18785.592900000003,29766.430800000006,31702.573800000002,31864.573800000002,31864.573800000002,31864.573800000002,31864.573800000002,31864.573800000002,31864.573800000002,31864.573800000002]
["Wind",9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,9364.1589999999942,null,null,"Wind",0,834.95500000000004,1419.5239999999999,1499.5239999999999,1499.5239999999999,1499.5239999999999,1499.5239999999999,1499.5239999999999,1499.5239999999999,1499.5239999999999,1499.5239999999999,null,null,"Wind",9364.1589999999942,10199.113999999994,10783.682999999994,10863.682999999994,10863.682999999994,10863.682999999994,10863.682999999994,10863.682999999994,10863.682999999994,10863.682999999994,10863.682999999994]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",475.41022461428071,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,null,null,"Conventional Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Conventional Hydro",475.41022461428071,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994,475.40653031933994]
["Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0]
["Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0]
["Nuclear",4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2,4973.2]
["Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hybrid",0,0,0,0,0,0,0,0,0,0,0]
["Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0]
["Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing - Western",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Western",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Western"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",23033.665426486165,21844.854928763176,20858.588642763178,20221.101056464548,16940.751958464545,16938.726358464544,15598.587208418743,14890.702437486827,14301.982391486827,14309.673171627017,12401.704499627018,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",23033.665426486165,21844.854928763176,20858.588642763178,20221.101056464548,16940.751958464545,16938.726358464544,15598.587208418743,14890.702437486827,14301.982391486827,14309.673171627017,12401.704499627018]
["Petroleum",809.48788100000002,809.02161800000067,809.71471400000087,812.02556900000002,812.02556900000002,812.02556900000002,812.02556900000002,810.05792299999973,810.05792299999973,809.75167199999953,809.75167199999953,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",809.48788100000002,809.02161800000067,809.71471400000087,812.02556900000002,812.02556900000002,812.02556900000002,812.02556900000002,810.05792299999973,810.05792299999973,809.75167199999953,809.75167199999953]
["Natural Gas and Other Gases",98357.012306533215,96853.232751866846,94009.126041066775,93837.893628066406,93681.450248066394,92238.353102066409,91637.54942206644,91478.475260866704,91144.110140866716,91009.519943866399,90780.736263866405,null,null,"Natural Gas and Other Gases",693.51341999999977,1989.6750200000006,3307.7998460000003,4963.5169810000007,4966.464081000001,5157.1323810000004,5161.666381,5045.1638459999995,5317.0074459999978,5413.6219359999977,5408.1811359999974,null,null,"Natural Gas and Other Gases",99050.525726533218,98842.907771866841,97316.925887066769,98801.410609066399,98647.914329066392,97395.485483066412,96799.215803066443,96523.6391068667,96461.11758686672,96423.141879866394,96188.917399866405]
["Biomass",2923.9995469999976,2910.2884979999985,2906.1501859999989,2905.0010770000013,2895.0177300000014,2867.6279500000014,2868.5124580000011,2796.5050639999954,2800.8086779999949,2799.6141049999997,2799.1638250000001,null,null,"Biomass",48.659066000000003,48.677279800000008,48.618442000000002,48.618442000000002,48.618442000000002,48.618442000000002,48.618442000000002,48.651472200000001,48.651472200000001,48.651472200000001,48.651472200000001,null,null,"Biomass",2972.6586129999978,2958.9657777999987,2954.7686279999989,2953.6195190000012,2943.6361720000014,2916.2463920000014,2917.130900000001,2845.1565361999956,2849.460150199995,2848.2655771999998,2847.8152972000003]
["Solar",18614.857194599954,18478.798789400007,17803.511958200008,17184.556663399966,17192.466799399968,17091.316639399967,16662.749119200023,17757.472008200009,17807.501928200007,17130.286937399964,16961.366729399968,null,null,"Solar",3783.750646,7794.1845720000001,10202.294685999999,10308.956176000003,10475.919876000004,10843.819776000004,10955.408521999998,11691.128386000002,11809.201386000002,11135.792826000004,11006.008776000004,null,null,"Solar",22398.607840599954,26272.983361400009,28005.806644200005,27493.512839399969,27668.386675399972,27935.136415399971,27618.157641200021,29448.60039420001,29616.703314200007,28266.079763399968,27967.37550539997]
["Wind",5919.119353000001,4876.6826020000017,4426.7072420000004,4773.2975160000005,4707.5371160000022,4712.6406160000015,5053.5278010000038,4303.5419069999998,4004.6608369999999,4389.6014510000032,4454.9391910000022,null,null,"Wind",435.07568800000001,474.45791800000001,650.55163799999991,652.23070800000005,639.90430800000001,650.03934800000002,675.50228800000002,650.55163799999991,534.68347799999992,601.69246799999996,650.03934800000002,null,null,"Wind",6354.1950410000009,5351.1405200000017,5077.2588800000003,5425.5282240000006,5347.4414240000024,5362.6799640000017,5729.0300890000035,4954.0935449999997,4539.3443150000003,4991.2939190000034,5104.9785390000025]
["Geothermal",4202.2568820000015,4198.9364360000009,4201.7246550000009,4203.7446160000018,4188.2525160000014,4188.2525160000014,4188.2525160000014,4161.2777889999998,4161.2777889999998,4167.4837700000026,4167.4837700000026,null,null,"Geothermal",60.072199999999995,470.11220000000003,470.38660000000004,470.57024999999999,470.57024999999999,470.57024999999999,470.57024999999999,470.81574999999998,470.81574999999998,473.84840000000003,473.84840000000003,null,null,"Geothermal",4262.3290820000011,4669.0486360000014,4672.1112550000007,4674.3148660000015,4658.8227660000011,4658.8227660000011,4658.8227660000011,4632.0935389999995,4632.0935389999995,4641.3321700000024,4641.3321700000024]
["Conventional Hydro",39312.487583570524,39582.937951084314,37064.083203506685,36261.48690986741,36061.167047605035,36855.307151977235,37998.141163627093,36968.501243768638,37804.076517693029,36845.916558538585,36831.596558538586,null,null,"Conventional Hydro",88.085369554339835,103.97154449913724,612.893267585128,727.97259829968095,749.85488920877197,846.64280346241958,850.3579664572577,838.32523354098271,912.20533589788533,912.77693589788544,912.77693589788544,null,null,"Conventional Hydro",39400.572953124865,39686.909495583452,37676.97647109181,36989.459508167092,36811.021936813806,37701.949955439653,38848.499130084354,37806.826477309623,38716.281853590917,37758.693494436469,37744.37349443647]
["Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0]
["Pumped Storage",2541.0602062102785,2549.9656948820607,1726.4048990229064,1707.5141118151532,1707.5141118151532,1707.5141118151532,2447.6413794286696,1726.4048990229064,1726.4048990229064,1707.5141118151532,1707.5141118151532,null,null,"Pumped Storage",59.339232736572882,75.197416879795398,75.197416879795398,69.394833759590796,69.394833759590796,69.394833759590796,59.339232736572882,75.197416879795398,75.197416879795398,69.394833759590796,69.394833759590796,null,null,"Pumped Storage",2600.3994389468512,2625.1631117618563,1801.6023159027018,1776.9089455747439,1776.9089455747439,1776.9089455747439,2506.9806121652423,1801.6023159027018,1801.6023159027018,1776.9089455747439,1776.9089455747439]
["Nuclear",7794.2483691072102,7794.6255674356398,7791.5837681644662,6686.2018681644677,5580.9368681644673,5580.9368681644673,5580.9368681644673,5575.2436756570114,5575.2436756570114,5569.6324756570111,5569.6324756570111,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",7794.2483691072102,7794.6255674356398,7791.5837681644662,6686.2018681644677,5580.9368681644673,5580.9368681644673,5580.9368681644673,5575.2436756570114,5575.2436756570114,5569.6324756570111,5569.6324756570111]
["Hybrid",401.18200000000002,401.11809999999997,400.77249999999998,400.81499999999994,400.81499999999994,400.81499999999994,400.81499999999994,401.11339999999996,401.11339999999996,401.35589999999996,401.35589999999996,null,null,"Hybrid",475.72500000000002,865.0311999999999,1278.1656,1276.7795000000001,1276.7795000000001,1276.7795000000001,1276.7795000000001,1278.8072,1278.8072,1279.0617,1279.0617,null,null,"Hybrid",876.90700000000004,1266.1492999999998,1678.9381000000001,1677.5945000000002,1677.5945000000002,1677.5945000000002,1677.5945000000002,1679.9205999999999,1679.9205999999999,1680.4176,1680.4176]
["Other",341.40390799999994,312.53156000000007,312.35482899999994,313.57676099999992,313.56289999999996,313.52890999999994,313.65936399999993,312.49688099999997,312.63858799999997,313.45971799999995,313.35305799999992,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",341.40390799999994,312.53156000000007,312.35482899999994,313.57676099999992,313.56289999999996,313.52890999999994,313.65936399999993,312.49688099999997,312.63858799999997,313.45971799999995,313.35305799999992]
["Battery",2603.7971799999987,2603.0931369999998,2601.60194,2601.5499999999997,2601.6149999999993,2601.5349999999994,2601.6349999999998,2603.4444629999989,2603.4844629999989,2603.6913429999991,2603.5713429999992,null,null,"Battery",1772.1439520000004,3625.4772119999989,4592.5177159999994,5619.2479809999995,5624.2479809999995,5629.2479809999995,6104.2479809999995,6108.7907559999985,6377.7822559999995,6376.4792560000014,6738.6197560000019,null,null,"Battery",4375.941131999999,6228.5703489999987,7194.1196559999989,8220.7979809999997,8225.8629809999984,8230.7829809999985,8705.8829809999988,8712.2352189999983,8981.2667189999993,8980.1705990000009,9342.1910990000015]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"Table J","index":11,"n_rows":77,"n_cols":40,"rows_kept":77,"cut":false,"hidden":false,"merged":[[3,28,3,39],[22,28,22,39],[41,28,41,39],[60,28,60,39],[3,0,3,11],[22,0,22,11],[41,0,41,11],[60,0,60,11],[3,14,3,25],[22,14,22,25],[41,14,41,25],[60,14,60,25]]}
[]
[null,null,null,null,null,null,"See Demand Assumptions and Resource Categories description in the 2022 LTRA for definitions of generating unit status tiers"]
[]
["Existing - Eastern",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Eastern",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Eastern"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",181664.46001090007,177146.06001090005,173406.76001090003,171447.41001090003,169542.41001090009,165010.51001090006,160094.51001090006,155292.51001090009,152520.51001090009,152520.51001090009,150197.51001090006,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",181664.46001090007,177146.06001090005,173406.76001090003,171447.41001090003,169542.41001090009,165010.51001090006,160094.51001090006,155292.51001090009,152520.51001090009,152520.51001090009,150197.51001090006]
["Petroleum",37391.090499999955,36460.19049999999,36473.970499999989,36243.270499999991,36016.470499999989,35758.870499999983,35758.870499999983,35758.870499999983,35528.870499999975,35485.470499999974,35485.470499999974,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",37391.090499999955,36460.19049999999,36473.970499999989,36243.270499999991,36016.470499999989,35758.870499999983,35758.870499999983,35758.870499999983,35528.870499999975,35485.470499999974,35485.470499999974]
["Natural Gas and Other Gases",369376.37600000104,369220.52600000118,366747.52600000118,362988.32600000111,361384.72600000113,358128.52600000118,356326.9260000012,356323.72600000113,356152.72600000119,354813.72600000113,354813.72600000113,null,null,"Natural Gas and Other Gases",1997.3489994049073,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,4140.3489994049069,null,null,"Natural Gas and Other Gases",371373.72499940597,373360.87499940611,370887.87499940611,367128.67499940604,365525.07499940606,362268.87499940611,360467.27499940613,360464.07499940606,360293.07499940612,358954.07499940606,358954.07499940606]
["Biomass",5059.4700000000066,5101.4700000000066,5026.9700000000075,4894.9700000000075,4894.9700000000075,4785.2700000000068,4751.2700000000068,4751.2700000000068,4716.2700000000068,4716.2700000000068,4716.2700000000068,null,null,"Biomass",0,0,0,0,0,0,0,0,0,0,0,null,null,"Biomass",5059.4700000000066,5101.4700000000066,5026.9700000000075,4894.9700000000075,4894.9700000000075,4785.2700000000068,4751.2700000000068,4751.2700000000068,4716.2700000000068,4716.2700000000068,4716.2700000000068]
["Solar",18573.727699999992,18673.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,18754.727699999992,null,null,"Solar",370.4,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,5125.6399999999994,null,null,"Solar",18944.127699999994,23799.367699999992,23880.367699999992,23880.367699999992,23880.367699999992,23880.367699999992,23880.367699999992,23880.367699999992,23880.367699999992,23880.367699999992,23880.367699999992]
["Wind",77647.066400000025,77715.566400000025,78476.516400000022,78448.516400000022,78428.716400000019,78336.716400000005,77994.866400000028,77869.866400000028,77697.476400000029,77654.896400000027,77654.896400000027,null,null,"Wind",0,935.12,935.12,935.12,935.12,935.12,935.12,935.12,935.12,935.12,935.12,null,null,"Wind",77647.066400000025,78650.686400000021,79411.636400000018,79383.636400000018,79363.836400000015,79271.8364,78929.986400000023,78804.986400000023,78632.596400000024,78590.016400000022,78590.016400000022]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",40576.198999999993,40699.698999999993,40699.698999999993,40699.698999999993,40699.698999999993,40699.698999999993,40699.698999999993,40669.698999999993,40669.698999999993,40489.198999999986,40489.198999999986,null,null,"Conventional Hydro",353.99999999999994,571.49999999999989,571.49999999999989,571.49999999999989,571.49999999999989,571.49999999999989,571.49999999999989,541.49999999999989,541.49999999999989,541.49999999999989,541.49999999999989,null,null,"Conventional Hydro",40930.198999999993,41271.198999999993,41271.198999999993,41271.198999999993,41271.198999999993,41271.198999999993,41271.198999999993,41211.198999999993,41211.198999999993,41030.698999999986,41030.698999999986]
["Run of River Hydro",2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988,2584.3193149999988]
["Pumped Storage",20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,20101.80000000001,null,null,"Pumped Storage",66,66,66,66,66,66,66,66,66,66,66,null,null,"Pumped Storage",20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001,20167.80000000001]
["Nuclear",96100.5,94438.5,96141.5,95211.5,95211.5,93987.5,93946.5,93946.5,94768.5,93999.9,93999.9,null,null,"Nuclear",0,1100,1100,1100,1100,1100,1100,1100,1100,1100,1100,null,null,"Nuclear",96100.5,95538.5,97241.5,96311.5,96311.5,95087.5,95046.5,95046.5,95868.5,95099.9,95099.9]
["Hybrid",40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,40.408799999999999,null,null,"Hybrid",0,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,19.899999999999999,null,null,"Hybrid",40.408799999999999,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998,60.308799999999998]
["Other",3282.64,3282.64,3282.64,3242.64,3207.64,3202.33,3202.33,3186.4,3186.4,3186.4,3186.4,null,null,"Other",0,485.5,485.5,485.5,485.5,485.5,485.5,485.5,485.5,485.5,485.5,null,null,"Other",3282.64,3768.14,3768.14,3728.14,3693.14,3687.83,3687.83,3671.9,3671.9,3671.9,3671.9]
["Battery",586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,586.99131800000009,null,null,"Battery",8.3000000000000007,112.8,748,814,814,1164,1564,2514,3114,4164,4164,null,null,"Battery",595.29131800000005,699.79131800000005,1334.9913180000001,1400.9913180000001,1400.9913180000001,1750.9913180000001,2150.9913180000003,3100.9913180000003,3700.9913180000003,4750.9913180000003,4750.9913180000003]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing - Quebec",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Quebec",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Quebec"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0]
["Petroleum",436,436,436,436,436,436,436,436,436,436,436,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",436,436,436,436,436,436,436,436,436,436,436]
["Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0,null,null,"Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0,null,null,"Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0]
["Biomass",338.88200000000001,330.78199999999998,330.78199999999998,330.78199999999998,330.78199999999998,275.78199999999998,208.232,208.232,208.232,208.232,200.63200000000001,null,null,"Biomass",9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,9.5,null,null,"Biomass",348.38200000000001,340.28199999999998,340.28199999999998,340.28199999999998,340.28199999999998,285.28199999999998,217.732,217.732,217.732,217.732,210.13200000000001]
["Solar",0,0,0,0,0,0,0,0,0,0,0,null,null,"Solar",0,0,0,0,0,0,0,0,0,0,0,null,null,"Solar",0,0,0,0,0,0,0,0,0,0,0]
["Wind",3715.7499999999995,3715.7499999999995,3715.7499999999995,3715.7499999999995,3606.2499999999995,3505.7499999999995,3396.2499999999995,3262.9499999999994,3262.9499999999994,3103.9499999999994,2422.6499999999996,null,null,"Wind",0,0,0,0,0,0,0,0,0,0,0,null,null,"Wind",3715.7499999999995,3715.7499999999995,3715.7499999999995,3715.7499999999995,3606.2499999999995,3505.7499999999995,3396.2499999999995,3262.9499999999994,3262.9499999999994,3103.9499999999994,2422.6499999999996]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,40010.725999999995,null,null,"Conventional Hydro",245,245,245,245,245,245,245,245,245,245,245,null,null,"Conventional Hydro",40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995]
["Run of River Hydro",103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,93.518000000000001,80.2,55.2,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,93.518000000000001,80.2,55.2]
["Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0]
["Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0]
["Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hybrid",0,0,0,0,0,0,0,0,0,0,0]
["Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0]
["Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing - Texas",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Texas",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Texas"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",14018.4,14672.39,14672.39,14672.39,14672.39,14672.39,14672.39,14672.39,14672.39,14672.39,14672.39,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0]
["Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",436,436,436,436,436,436,436,436,436,436,436]
["Natural Gas and Other Gases",55327.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,55509.946999999964,null,null,"Natural Gas and Other Gases",0,492.8,522.80000000000007,522.80000000000007,522.80000000000007,522.80000000000007,522.80000000000007,432.8,0,522.80000000000007,522.80000000000007,null,null,"Natural Gas and Other Gases",0,0,0,0,0,0,0,0,0,0,0]
["Biomass",174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,174.24999999999997,null,null,"Biomass",0,0,0,0,0,0,0,0,0,0,0,null,null,"Biomass",348.38200000000001,340.28199999999998,340.28199999999998,340.28199999999998,340.28199999999998,285.28199999999998,217.732,217.732,217.732,217.732,210.13200000000001]
["Solar",11603.1,11603.1,11603.1,11603.1,11603.1,11603.1,11603.1,11603.1,11603.1,11603.1,11603.1,null,null,"Solar",0,11607.990000000002,25164.579999999994,27554.879999999994,27754.879999999994,27754.879999999994,27754.879999999994,3840.41,0,27754.879999999994,27754.879999999994,null,null,"Solar",0,0,0,0,0,0,0,0,0,0,0]
["Wind",35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,35248.929999999993,null,null,"Wind",0,3363.7000000000003,5358.5000000000009,5758.5,5758.5,5758.5,5758.5,2170.1,0,5758.5,5758.5,null,null,"Wind",3715.7499999999995,3715.7499999999995,3715.7499999999995,3715.7499999999995,3606.2499999999995,3505.7499999999995,3396.2499999999995,3262.9499999999994,3262.9499999999994,3103.9499999999994,2422.6499999999996]
["Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Geothermal",0,0,0,0,0,0,0,0,0,0,0]
["Conventional Hydro",545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,545.3900000000001,null,null,"Conventional Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Conventional Hydro",40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995,40255.725999999995]
["Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,103.41800000000001,93.518000000000001,80.2,55.2]
["Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0,null,null,"Pumped Storage",0,0,0,0,0,0,0,0,0,0,0]
["Nuclear",5268,5268,5268,5268,5268,5268,5268,5268,5268,5268,5268,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0]
["Hybrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hyrbrid",0,0,0,0,0,0,0,0,0,0,0,null,null,"Hyrbrid",0,0,0,0,0,0,0,0,0,0,0]
["Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0]
["Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0,null,null,"Battery",0,0,0,0,0,0,0,0,0,0,0]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing - Western",null,null,null,null,null,null,null,null,null,null,null,null,null,"Tier 1 - Western",null,null,null,null,null,null,null,null,null,null,null,null,null,"Existing and Tier 1 - Western"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,null,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",25586.706335877854,24280.206335877858,23033.176335877859,22137.28633587786,18514.626335877863,18514.626335877863,16997.620000000003,16223.660000000002,15562.880000000001,15562.880000000001,13397.140000000001,null,null,"Coal",0,0,0,0,0,0,0,0,0,0,0,null,null,"Coal",25586.706335877854,24280.206335877858,23033.176335877859,22137.28633587786,18514.626335877863,18514.626335877863,16997.620000000003,16223.660000000002,15562.880000000001,15562.880000000001,13397.140000000001]
["Petroleum",876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,null,null,"Petroleum",0,0,0,0,0,0,0,0,0,0,0,null,null,"Petroleum",876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986,876.89999999999986]
["Natural Gas and Other Gases",105479.96199999968,103920.41199999968,100843.56199999967,100654.06199999967,100464.56199999967,98932.301999999661,98238.901999999798,98128.901999999798,97741.221999999805,97581.821999999811,97353.821999999811,null,null,"Natural Gas and Other Gases",718.6,2071.3999999999996,3679.4300000000003,5329.4299999999994,5329.4299999999994,5544.4299999999994,5544.4299999999994,5544.4299999999994,5844.43,5844.43,5844.43,null,null,"Natural Gas and Other Gases",106198.56199999969,105991.81199999967,104522.99199999968,105983.49199999966,105793.99199999966,104476.73199999965,103783.33199999979,103673.33199999979,103585.6519999998,103426.2519999998,103198.2519999998]
["Biomass",3015.9800000000014,3003.1800000000021,2999.9000000000015,2997.4000000000015,2991.1500000000015,2961.1500000000015,2961.1500000000015,2896.3500000000013,2896.3500000000013,2896.3500000000013,2894.7500000000014,null,null,"Biomass",51.244,51.244,51.244,51.244,51.244,51.244,51.244,51.244,51.244,51.244,51.244,null,null,"Biomass",3067.2240000000015,3054.4240000000023,3051.1440000000016,3048.6440000000016,3042.3940000000016,3012.3940000000016,3012.3940000000016,2947.5940000000014,2947.5940000000014,2947.5940000000014,2945.9940000000015]
["Solar",26091.659000000025,26091.659000000025,26091.659000000025,26091.659000000025,26091.659000000025,26041.659000000025,26032.709000000024,26032.709000000024,26032.709000000024,26011.709000000024,25845.969000000019,null,null,"Solar",5378.91,10789.52,14412.020000000004,15151.520000000004,15382.520000000004,16191.520000000004,16321.520000000004,16431.520000000004,16441.520000000004,16441.520000000004,16441.520000000004,null,null,"Solar",31470.569000000025,36881.179000000026,40503.679000000033,41243.179000000033,41474.179000000033,42233.179000000033,42354.229000000028,42464.229000000028,42474.229000000028,42453.229000000028,42287.489000000023]
["Wind",32179.040000000005,32149.350000000006,32108.350000000006,32108.350000000006,31980.650000000005,31980.650000000005,31404.150000000005,31340.7,31126.3,30862.1,30504.699999999997,null,null,"Wind",2916.32,3596.92,4557.92,4557.92,4557.92,4557.92,4557.92,4557.92,4557.92,4557.92,4557.92,null,null,"Wind",35095.360000000008,35746.270000000004,36666.270000000004,36666.270000000004,36538.570000000007,36538.570000000007,35962.070000000007,35898.620000000003,35684.22,35420.019999999997,35062.619999999995]
["Geothermal",4506.95,4506.95,4506.95,4506.95,4489.95,4489.95,4489.95,4463.45,4463.45,4463.45,4463.45,null,null,"Geothermal",66,520.5,520.5,520.5,520.5,520.5,520.5,520.5,520.5,520.5,520.5,null,null,"Geothermal",4572.95,5027.45,5027.45,5027.45,5010.45,5010.45,5010.45,4983.95,4983.95,4983.95,4983.95]
["Conventional Hydro",71684.616199999815,71395.396199999828,71064.916199999818,71077.586199999831,70913.446199999831,70896.496199999849,70866.436199999851,70866.436199999851,70866.436199999851,70852.366199999829,70852.366199999829,null,null,"Conventional Hydro",188.06,210.56,1164.7100000000003,1355.5400000000002,1410.4400000000003,1465.3400000000001,1520.2400000000002,1575.1400000000003,1575.1400000000003,1575.1400000000003,1575.1400000000003,null,null,"Conventional Hydro",71872.676199999813,71605.956199999826,72229.626199999824,72433.126199999824,72323.886199999833,72361.836199999845,72386.676199999856,72441.57619999985,72441.57619999985,72427.506199999829,72427.506199999829]
["Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0,null,null,"Run of River Hydro",0,0,0,0,0,0,0,0,0,0,0]
["Pumped Storage",4577.67,4577.67,4577.67,4577.67,4577.67,4577.67,4577.67,4577.67,4577.67,4577.67,4577.67,null,null,"Pumped Storage",162,162,162,162,162,162,162,162,162,162,162,null,null,"Pumped Storage",4739.67,4739.67,4739.67,4739.67,4739.67,4739.67,4739.67,4739.67,4739.67,4739.67,4739.67]
["Nuclear",8427.57,8427.57,8427.57,7277.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,null,null,"Nuclear",0,0,0,0,0,0,0,0,0,0,0,null,null,"Nuclear",8427.57,8427.57,8427.57,7277.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006,6127.5700000000006]
["Hybrid",428,428,428,428,428,428,428,428,428,428,428,null,null,"Hybrid",510,931,1404,1404,1404,1404,1404,1404,1404,1404,1404,null,null,"Hybrid",938,1359,1832,1832,1832,1832,1832,1832,1832,1832,1832]
["Other",361.1,329.3,329.3,329.3,329.3,329.3,329.3,329.3,329.3,329.3,329.3,null,null,"Other",0,0,0,0,0,0,0,0,0,0,0,null,null,"Other",361.1,329.3,329.3,329.3,329.3,329.3,329.3,329.3,329.3,329.3,329.3]
["Battery",2764.76,2764.76,2764.76,2764.76,2764.76,2764.76,2764.76,2764.76,2764.76,2764.76,2764.76,null,null,"Battery",1904.46,3926.96,5034.96,6139.11,6144.11,6149.11,6624.11,6624.11,6907.11,6907.11,7288.11,null,null,"Battery",4669.22,6691.72,7799.72,8903.869999999999,8908.869999999999,8913.869999999999,9388.869999999999,9388.869999999999,9671.869999999999,9671.869999999999,10052.869999999999]
["Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0,null,null,"Unknown",0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"Table K","index":12,"n_rows":5,"n_cols":26,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,11],[0,13,0,25]]}
["Ten Year Historical Transmission Projects by Circuit Miles",null,null,null,null,null,null,null,null,null,null,null,null,"Future Transmission Circuit Miles > 100 kV by Project Status"]
[null,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,null,null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,"Not Dated"]
["Total",39779,38813,32718,33262,32718,19888,15723,18253.160598839997,15022.632311378697,15268.154028799998,17650.11398461106,null,"Under Construction",596.40999999999985,815.8599999999999,911.18999999999994,924.43999999999994,968.43999999999994,1032.28,1032.28,1032.28,1032.28,1032.28,1032.28,1032.28]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Planned",970.87999999999988,3685.7570853568686,5926.0079504904961,7270.9418846110693,9520.0418846110606,10590.631884611061,10970.021884611058,11355.161884611058,11636.141884611057,11697.041884611059,11764.041884611059,11809.16188461106]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Conceptual",201.84,763.74,956.51,1146.6300000000001,1577.93,1816.7021,1888.3020999999999,2392.0520999999999,3404.4520999999995,3415.4520999999995,3854.4520999999995,4808.6720999999998]

{"sheet":"Table L","index":13,"n_rows":11,"n_cols":13,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["kV",2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,"Not Dated"]
["100-120",520.18000000000006,851.54902423865769,1320.556738346799,1601.6097464263514,1923.1397464263514,2155.289746426351,2293.5097464263508,2328.6497464263502,2386.7497464263506,2447.6497464263512,2514.6497464263512,2680.9097464263514]
["121-150",255.35000000000002,635.18910000000005,722.18910000000005,835.22910000000002,839.22910000000002,915.34120000000007,988.34120000000007,988.34120000000007,994.34120000000007,1005.3412000000001,1005.3412000000001,1005.3412000000001]
["151-199",211.6,265.45,412.53,519.92092604101924,680.67092604101924,744.51092604101927,744.51092604101927,796.26092604101927,813.76092604101927,813.76092604101927,813.76092604101927,813.76092604101927]
["200-299",372.79,917.54171231820976,1914.5848633436906,2229.4448633436905,2574.5448633436908,2920.6448633436912,3136.4148633436912,3250.4148633436912,3345.3148633436913,3345.3148633436913,3345.3148633436913,3573.3948633436912]
["300-399",280.70000000000005,1368.92,1631.2200000000003,2185.61,2403.0099999999998,2683.0099999999998,2683.0099999999998,2683.0099999999998,2904.89,2904.89,3043.89,3151.89]
["400-599",128.51,1071.4072487999999,1637.3272487999998,1814.8972487999999,3478.5172487999998,3853.5172487999998,3877.5172487999998,4565.5172487999998,5460.5172488000007,5460.5172488000007,5760.5172488000007,6257.5172488000007]
["600+",0,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001,155.30000000000001]

{"sheet":"Table M","index":14,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,"10-50","51-100","101-200","201-300","300+"]
["MISO",306.84999999999997,60,0,0,0]
["MRO-Manitoba",103,80,0,0,0]
["NPCC-Maritimes",23.612100000000002,0,0,0,0]
["MRO-SaskPower",63,371,0,0,0]
["NPCC-New England",149.69999999999999,59,0,207,0]
["NPCC-New York",786.26,461.8,0,0,1046]
["NPCC-Ontario",71,135,228,236,0]
["NPCC-Quebec",37,0,279.60000000000002,0,0]
["PJM",944.1,220.4,230,0,0]
["SERC-C",199.92000000000002,0,0,0,0]
["SERC-E",189.77999999999997,0,0,0,0]
["SERC-FP",134.57999999999998,51.44,0,0,0]
["SERC-SE",258.91999999999996,194.1,176,0,0]
["SPP",147.10000000000002,0,123,0,0]
["Texas RE-ERCOT",288.8,55.2,0,0,0]
["WECC-AB",129.8938799999998,63.379899999999999,127.7290228,0,0]
["WECC-BC",143,172,175,279,0]
["WECC-CA/MX",529.59971410814171,370.87800497203222,125,0,0]
["WECC-WPP",0,0,0,0,0]
["WECC-SRSG",778.15,422.42,288,0,500]
["Total",5284.2656941081414,2716.6179049720322,1752.3290227999998,722,1546]

{"sheet":"Table N","index":15,"n_rows":11,"n_cols":13,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,"Not Dated"]
["Economics / Congestion",239.43,418.87,1490.09,1751.66,2099.2799999999997,2478.6800000000003,2478.6800000000003,2478.6800000000003,2487.5800000000004,2487.5800000000004,2487.5800000000004,2487.5800000000004]
["Fossil-Fired Integration",0,131,131,131,131,131,131,131,131,131,131,131.08000000000001]
["Hydro Integration",0,0,0,10,10,10,10,10,10,10,10,10]
["Nuclear Integration",0,0,0,0,0,0,0,0,0,0,0,0]
["Other",-91.780000000000015,279.8599999999999,384.8599999999999,398.64999999999986,1580.6499999999994,1581.8999999999994,1672.8999999999994,1672.8999999999994,2370.8999999999996,2370.8999999999996,2809.8999999999996,2809.8999999999996]
["Reliability",1598.6299999999997,3590.5601565568686,4964.5310216904927,5944.3749558110658,7058.8949558110708,7850.9470558110697,8227.9370558110713,9016.8270558110707,9328.3070558110721,9412.2070558110718,9479.2070558110718,10262.467055811072]
["Variable/Renewable Integration",43.65,1178.8669287999999,1260.0269287999995,1588.0269287999995,1724.0869287999999,2004.0869287999999,2004.0869287999999,2107.0869287999999,2382.0869287999999,2382.0869287999999,2382.0869287999999,2598.0869287999999]

{"sheet":"Table O","index":16,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,1,1,7],[2,1,3,1],[2,2,2,4],[2,5,2,7]]}
[]
[null,"BPS Wind and Solar Generation Resources by Assessment Area Year 2022"]
[null,"Nameplate (MW)","Wind",null,null,"Solar"]
[null,null,"Nameplate (MW)","Available Peak Demand Hour Capacity (MW)","Available/Nameplate (%)","Nameplate (MW)","Available Peak Demand Hour Capacity (MW)","Available/Nameplate (%)"]
[null,"MISO",25270.592000000001,4209.4684000000016,0.16657577313582528,1768.65,1079.9999999999998,0.61063523026036792]
[null,"MRO-Manitoba Hydro",0,0,"-",0,0,"-"]
[null,"MRO-SaskPower",626.6,62.44,9.9648898819023293E-2,25.599999999999998,0,"-"]
[null,"NPCC-Maritimes",1210.4000000000001,228.59000000000003,0.18885492399206874,10.24,0.86,8.3984375E-2]
[null,"NPCC-New England",1503.8163999999995,201.15699999999987,0.1337643345291353,2315.9506999999971,276.18730000000011,0.1192543951820738]
[null,"NPCC-New York",1897.3000000000002,277.76999999999992,0.14640278290201861,51.5,21.4,0.41553398058252422]
[null,"NPCC-Ontario",4783.0119999999988,746.14987200000007,0.15600000000000006,478,123.13400000000001,0.25760251046025107]
[null,"NPCC-Quebec",3715.7499999999995,0,0,9.5,0,"-"]
[null,"PJM",11013.2,1511.4,0.13723531761885738,4988.473,2393.7800000000011,0.47986227448760393]
[null,"SERC-C",964.4,957.78,0.99313562836997094,449.77999999999992,287.01999999999992,0.63813419894170476]
[null,"SERC-E",0,0,"-",726.53,717.69,0.98783257401621416]
[null,"SERC-FP",0,0,"-",5544.5599999999995,3324.2599999999993,0.59955343616084944]
[null,"SERC-SE",0,0,"-",3775.3899999999994,3283.1000000000004,0.86960552419750037]
[null,"SPP",30264.3,6088.2246007000012,0.20116852531530555,312.77999999999992,148.67999999999998,0.47535008632265496]
[null,"Texas RE-ERCOT",35690.33,9364.1589999999942,0.26237244093848372,11603.1,9383.1210000000028,0.80867363032293116]
[null,"WECC-AB",2269,158.14930000000001,6.9699999999999998E-2,336,281.60159999999996,0.83809999999999985]
[null,"WECC-BC",717,68.975399999999993,9.6199999999999994E-2,2.04,1.709724,0.83809999999999996]
[null,"WECC-CA/MX",8828.25,1905.0679299999999,0.21579224987964771,17010.701999999994,11620.210751399982,0.68311176995517209]
[null,"WECC-WPP",18564.179999999993,2474.6399130000009,0.13330187021457462,6315.3189999999959,4857.4586289999934,0.76915491188964435]
[null,"WECC-SRSG",1800.6100000000001,269.85005899999999,0.1498659115521962,2427.5980000000004,1717.8180850000001,0.7076204894714857]

{"sheet":"Table P","index":17,"n_rows":24,"n_cols":23,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,1,1,5],[1,6,1,10],[1,13,1,17],[1,18,1,22],[0,12,0,22],[0,0,0,10]]}
["Demand Response - Year 1",null,null,null,null,null,null,null,null,null,null,null,"Demand Response - Year 5"]
[null,"Summer ",null,null,null,null,"Winter",null,null,null,null,null,null,"Summer ",null,null,null,null,"Winter"]
[null,2018,2019,2020,2021,2022,2018,2019,2020,2021,2022,null,null,2018,2019,2020,2021,2022,2018,2019,2020,2021,2022]
["Demand Response - MISO Year 1",5990.4,5959.1826011999992,5801.2143137825396,6316.7984544274941,6158.3148058172937,3592.5593092840218,5212.4000000000024,4490.3559719029317,3483.6822060101308,5767.8,null,"Demand Response - MISO Year 5",5990.4,6014.1426011999984,5726.1878936140529,6507.9721852078746,6131.0595775554539,3592.5593092840218,5227.2,4556.9480102742673,3579.0798883760294,6839.4000000000033]
["Demand Response - MRO-Manitoba Year 1",0,0,0,0,0,0,0,0,0,0,null,"Demand Response - MRO-Manitoba Year 5",0,0,0,0,0,0,0,0,0,0]
["Demand Response - MRO-SaskPower Year 1",85,85,60,63,67,85,85,60,63,67,null,"Demand Response - MRO-SaskPower Year 5",85,85,60,63,67,85,85,60,63,67]
["Demand Response - NPCC-Maritimes Year 1",346.8,346.9,344.5,353.4,368.89883108212803,264.60000000000002,277.3,266.20000000000027,309.5,377.11900872905971,null,"Demand Response - NPCC-Maritimes Year 5",350.2,353.7,355.40000000000009,361.8,302.22679197953585,263.5,276.3,272.30000000000018,343.1,335.83241490518321]
["Demand Response - NPCC-New England Year 1",464.42599999999993,441.22100000000006,654.43600000000004,682.03600000000006,592.04299999999967,467.16099999999989,434.291,655.07600000000014,682.67600000000004,592.04299999999967,null,"Demand Response - NPCC-New England Year 5",624.44499999999994,685.55399999999997,592.04299999999989,677.67300000000012,765.35,623.15099999999995,685.55399999999997,592.04299999999989,678.86500000000012,765.35000000000025]
["Demand Response - NPCC-New York Year 1",870.5,903.7,876.5,822.1,812.5,636.9,595.6,579.4,433.5,484.7,null,"Demand Response - NPCC-New York Year 5",870.5,903.7,876.5,822.1,812.5,636.9,595.6,579.4,433.5,484.7]
["Demand Response - NPCC-Ontario Year 1",533,794.30814814814823,468.71180000000004,621.0569999999999,850.19999999999993,544.95000000000005,924.19063474025768,582.58789999999999,770.62280280891525,719.92940481465075,null,"Demand Response - NPCC-Ontario Year 5",549.45000000000005,794.30814814814823,468.71180000000004,511.64,367.2,544.95000000000005,924.19063474025768,582.58789999999999,770.62280280891525,524.92940481465075]
["Demand Response - NPCC-Ontario Year 1",0,0,0,0,0,2423.5,2748.3107669565197,2565.0236062133881,2586.7355458844609,3348.1700722810324,null,"Demand Response - NPCC-Ontario Year 5",0,0,0,0,0,2543.5,4072.1122442110104,3479.8116075871526,3758.3038044097443,4181.1222730759237]
["Demand Response - PJM Year 1",9113,9127,8955,8824,7065,791,8233,8120,8512,6730,null,"Demand Response - PJM Year 5",7747,9243,9172,8927,7167,6934,8386,8335,8619,6832]
["Demand Response - SERC-C Year 1",1795,2076,1958,1691,1786,1663,1967,1797,1515,1762,null,"Demand Response - SERC-C Year 5",1705,1894,1792,1690,1638,1501,1815,1716,1520,1654]
["Demand Response - SERC-E Year 1",1090,1068,955,969,1284,948,966,887,894,1272,null,"Demand Response - SERC-E Year 5",1093,1075,976,994,1130,951,973,910,916,1142]
["Demand Response - SERC-FP Year 1",3047,3104,2951,1258,2949,3053,2978,2759,1581,2892,null,"Demand Response - SERC-FP Year 5",3230,3300,3146,1289,3064,3178,3149,2931,1599,3035]
["Demand Response - SERC-SE Year 1",2101,2466,2354,1707,1197,2112,2478,2366,1718,1206,null,"Demand Response - SERC-SE Year 5",2103,2605,2556,1793,2222,2118,2621,2573,1805,2231]
["Demand Response - SPP Year 1",867.2,1077.74,605.66,729.3,730,428.2,223.4,223.2,210.8,209.4,null,"Demand Response -SPP Year 5",865.5,1167.26,683.51,993.5,943.1,404.2,206.4,222.2,210.8,195]
["Demand Response - Texas RE-ERCOT Year 1",2173,2251.4405781093692,2254,2032.6,2749.7751600000001,1891,2733.4494472781089,2807,2651.5,2686.33932,null,"Demand Response - Texas RE-ERCOT Year 5",2173,2230.6511724209076,2201,2032.6,2749.7751600000001,1891,2783.8583929579718,2807,2651.5,2686.33932]
["Demand Response - WECC-AB Year 1",0,0,0,0,0,0,0,0,0,0,null,"Demand Response - WECC-AB Year 5",0,0,0,0,0,0,0,0,0,0]
["Demand Response - WECC-BC Year 1",0,0,0,0,0,0,0,0,0,0,null,"Demand Response - WECC-BC Year 5",0,0,0,0,0,0,0,0,0,0]
["Demand Response - WECC-CAMX Year 1",969.5,910.34666397571561,1008.15454185009,928.16308602504739,861.75909976294929,806.17,808.98460283279417,847.7985030412674,814.56724084291454,768.62803343412315,null,"Demand Response - WECC-CAMX Year 5",925.74,904.72370042800901,972.29885983467102,928.16308602504739,928.31167414197535,771.28,805.0589590013027,872.46081590652466,814.56724084291454,821.36579729349046]
["Demand Response - WECC-SRSG Year 1",186.17,144.44447246171833,62.058,392.28611710241609,421.08753426999897,143.94999999999999,126.40075722866764,62.003999999999998,286.68870328562207,326.3824198261816,null,"Demand Response - WECC-SRSG Year 5",186.17,144.44447246171833,62.058,317.28611710241609,409.08753426999897,143.94999999999999,126.40075722866764,62.003999999999998,320.68870328562207,359.3824198261816]
["Demand Response - WECC-WPP Year 1",1212,868,1161.5,1335.6002634057313,1602.7651658336633,601,546,553.5,567.34026340573132,720.58343700740409,null,"Demand Response - WECC-WPP Year 5",1231,914,1179.5,1353.6310868619103,1685.1061224815835,594,569,571.5,580.37108686191027,737.08487983015914]
["Demand Response - All BPS Year 1",{"$f":"SUM(B4:B23)","v":30843.995999999999},{"$f":"SUM(C4:C23)","v":31623.283463894953},30469.73465563263,28725.340920960691,29495.34359676603,20451.990309284021,31337.327209036353,29621.145981157588,27080.612762237775,29930.094696092456,null,"Demand Response - All BPS Year 5",{"$f":"SUM(N4:N23)","v":29729.404999999999},32314.484094658783,30819.209553448723,29262.36547519725,30381.716860428547,26775.990309284021,33300.674988139217,31123.255333767946,28663.398526585133,32891.506509745588]

{"sheet":"Figure 5 - NP","index":18,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":true,"merged":[[4,0,4,11],[23,0,23,11],[42,0,42,11]]}
[]
[]
[]
[]
["Existing"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",221269.56634677804,216098.65634677801,211112.32634677793,208257.08634677797,202729.42634677797,198197.52634677794,191764.52001090004,186188.56001090008,182755.78001090008,182755.78001090008,178267.04001090009]
["Petroleum",38703.990499999956,37773.090499999977,37786.870499999975,37556.170499999978,37329.37049999999,37071.770499999984,37071.770499999984,37071.770499999984,36841.770499999984,36798.370499999983,36798.370499999983]
["Natural Gas and Other Gases",530184.28500000224,528650.88500000245,523101.03500000271,519152.33500000264,517359.23500000266,512570.77500000276,510075.77500000224,509962.57500000228,509403.89500000229,507905.49500000215,507677.49500000215]
["Biomass",8588.582000000024,8617.7820000000156,8531.9020000000219,8397.4020000000201,8391.1520000000201,8251.452000000023,8147.4520000000248,8033.8520000000244,7995.1020000000244,7995.1020000000244,7993.5020000000241]
["Solar",56268.486699999994,56368.486699999994,56449.486699999994,56449.486699999994,56449.486699999994,56399.486699999994,56390.536699999997,56390.536699999997,56390.536699999997,56369.536699999997,56203.796699999992]
["Wind",145075.03639999981,145113.84639999981,145833.79639999979,145805.79639999979,145658.29639999976,145566.29639999976,144647.94639999978,144459.4963999998,144072.70639999982,143765.92639999979,143408.5263999998]
["Geothermal",4506.95,4506.95,4506.95,4506.95,4489.95,4489.95,4489.95,4463.45,4463.45,4463.45,4463.45]
["Conventional Hydro",152816.93120000063,152651.21120000063,152320.73120000059,152333.4012000006,152169.26120000062,152152.31120000058,152122.25120000058,152092.25120000058,152092.25120000058,151897.6812000006,151897.6812000006]
["Run of River Hydro",2687.7373149999989,2687.7373149999989,2687.7373149999989,2687.7373149999989,2687.7373149999989,2687.7373149999989,2687.7373149999989,2687.7373149999989,2687.7373149999989,2672.5193149999986,2664.5193149999986]
["Pumped Storage",24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012,24679.470000000012]
["Nuclear",109796.07000000002,108134.07000000002,109837.07000000002,107757.07000000002,106607.07000000002,105383.07000000002,105342.07000000002,105342.07000000002,106164.07000000002,105395.47000000002,105395.47000000002]
["Hybrid",468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999,468.40879999999999]
["Other",3643.74,3611.9399999999996,3611.9399999999996,3571.9399999999996,3536.9399999999996,3531.6299999999997,3531.6299999999997,3515.7,3515.7,3515.7,3515.7]
["Battery",2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001,2923.7513180000001]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Tier 1"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",0,0,0,0,0,0,0,0,0,0,0]
["Petroleum",0,0,0,0,0,0,0,0,0,0,0]
["Natural Gas and Other Gases",2715.9489994049072,13326.388999176024,20865.618999176026,24597.718999176017,26137.818999176023,28262.818999176023,31123.818999176023,34813.818999176008,35570.818999176008,36027.818999176008,38325.818999176001]
["Biomass",51.244,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001,130.42400000000001]
["Solar",5899.31,46337.195000000007,76830.034998855612,82064.394998855627,83491.394998855641,84970.894998855641,85920.394998855627,86998.894998855612,87977.394998855627,89020.394998855598,89094.894998855598]
["Wind",5616.32,16122.039999999999,22010.139999999996,28045.34,29725.34,30605.34,30605.34,30605.34,30605.34,30605.34,30605.34]
["Geothermal",66,520.5,520.5,520.5,520.5,520.5,520.5,520.5,520.5,520.5,520.5]
["Conventional Hydro",542.06000000000006,1039.1599999999999,2002.8099999999997,2205.6399999999994,2260.5399999999995,2367.7599999999998,2422.66,2447.56,2447.56,2447.56,2447.56]
["Run of River Hydro",0,0,0,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003,40.700000000000003]
["Pumped Storage",228,228,228,228,228,228,228,228,228,228,228]
["Nuclear",0,2200,2200,2200,2200,2200,2200,2200,2200,2200,2200]
["Hybrid",510,2858.8,3457.7719999999999,3457.7719999999999,3457.7719999999999,3457.7719999999999,3457.7719999999999,3457.7719999999999,3457.7719999999999,3457.7719999999999,3457.7719999999999]
["Other",0,805.5,865.5,865.5,865.5,865.5,865.5,865.5,865.5,865.5,865.5]
["Battery",1402.76,3088.76,4358.96,5529.11,5534.11,5889.1100000000006,6764.1100000000006,7714.1100000000006,8597.11,9647.11,10028.11]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]
[]
[]
["Existing + Tier 1"]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["Coal",221269.56634677804,216098.65634677801,211112.32634677793,208257.08634677797,202729.42634677797,198197.52634677794,191764.52001090004,186188.56001090008,182755.78001090008,182755.78001090008,178267.04001090009]
["Petroleum",38703.990499999956,37773.090499999977,37786.870499999975,37556.170499999978,37329.37049999999,37071.770499999984,37071.770499999984,37071.770499999984,36841.770499999984,36798.370499999983,36798.370499999983]
["Natural Gas and Other Gases",532900.23399940715,541977.27399917843,543966.65399917879,543750.05399917869,543497.05399917869,540833.59399917873,541199.59399917827,544776.39399917831,544974.71399917826,543933.31399917812,546003.31399917812]
["Biomass",8639.8260000000246,8748.2060000000165,8662.3260000000228,8527.8260000000209,8521.5760000000209,8381.8760000000239,8277.8760000000257,8164.2760000000244,8125.5260000000244,8125.5260000000244,8123.926000000024]
["Solar",62167.796699999992,102705.6817,133279.52169885562,138513.88169885561,139940.88169885564,141370.38169885564,142310.93169885562,143389.43169885559,144367.93169885562,145389.93169885559,145298.6916988556]
["Wind",150691.35639999982,161235.88639999981,167843.93639999977,173851.13639999978,175383.63639999976,176171.63639999976,175253.28639999978,175064.8363999998,174678.04639999982,174371.26639999979,174013.8663999998]
["Geothermal",4572.95,5027.45,5027.45,5027.45,5010.45,5010.45,5010.45,4983.95,4983.95,4983.95,4983.95]
["Conventional Hydro",153358.99120000063,153690.37120000063,154323.54120000059,154539.04120000062,154429.80120000063,154520.07120000059,154544.91120000058,154539.81120000058,154539.81120000058,154345.2412000006,154345.2412000006]
["Run of River Hydro",2687.7373149999989,2687.7373149999989,2687.7373149999989,2728.4373149999988,2728.4373149999988,2728.4373149999988,2728.4373149999988,2728.4373149999988,2728.4373149999988,2713.2193149999985,2705.2193149999985]
["Pumped Storage",24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012,24907.470000000012]
["Nuclear",109796.07000000002,110334.07000000002,112037.07000000002,109957.07000000002,108807.07000000002,107583.07000000002,107542.07000000002,107542.07000000002,108364.07000000002,107595.47000000002,107595.47000000002]
["Hybrid",978.40879999999993,3327.2088000000003,3926.1808000000001,3926.1808000000001,3926.1808000000001,3926.1808000000001,3926.1808000000001,3926.1808000000001,3926.1808000000001,3926.1808000000001,3926.1808000000001]
["Other",3643.74,4417.4399999999996,4477.4399999999996,4437.4399999999996,4402.4399999999996,4397.1299999999992,4397.1299999999992,4381.2,4381.2,4381.2,4381.2]
["Battery",4326.5113179999998,6012.5113180000008,7282.7113179999997,8452.8613179999993,8457.8613179999993,8812.8613180000011,9687.8613180000011,10637.861318000001,11520.861318000001,12570.861318000001,12951.861318000001]
["Unknown",0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"Stacked DER-BTM","index":19,"n_rows":33,"n_cols":28,"rows_kept":33,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
["REGION","DEMAND-SIDE MANAGEMENT","Year(s)","Unit","2021 (S)","2022 (S)","2023 (S)","2024 (S)","2025 (S)","2026 (S)","2027 (S)","2028 (S)","2029 (S)","2030 (S)","2031 (S)","2032 (S)","2021-22 (W)","2022-23 (W)","2023-24 (W)","2024-25 (W)","2025-26 (W)","2026-27 (W)","2027-28 (W)","2028-29 (W)","2029-30 (W)","2030-31 (W)","2031-32 (W)","2032-33 (W)"]
["MISO","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,861,861,861,861,861,861,861,861,861,861,861,0,861,861,861,861,861,861,861,861,861,861,861]
["MRO-Manitoba","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,37.6,39.799999999999997,42,44.287840750000001,47.047959550886198,50.376201833676802,54.387111199688661,59.217232692323051,65.028839998365683,72.014062548563501,80.400000000000006,0,37.6,39.799999999999997,42,44.287840750000001,47.047959550886198,50.376201833676802,54.387111199688661,59.217232692323051,65.028839998365683,72.014062548563501,80.400000000000006]
["MRO-SaskPower","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,36,39,42,45,48,51,51,51,51,51,51,0,36,39,42,45,48,51,51,51,51,51,51]
["NPCC-Maritimes","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,69.766739362876336,90.672519966648238,109.16480684378509,126.10337329119324,145.83404359531727,169.98355360230761,198.13311156213189,231.00428769003841,268.89335990349497,302.91764867286224,326.99265541172912,0,87.672519966648238,108.16480684378509,125.10337329119324,145.83404359531727,168.98355360230761,197.13311156213189,230.00428769003841,267.89335990349497,301.91764867286224,325.99265541172912,348.82779044685105]
["NPCC-New England","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,3146,3500,3870,4239,4669,5009,5333,5648,5948,6244,6555,0,0,0,0,0,0,0,0,0,0,0,0]
["NPCC-New York","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,3896,4710.5,5611.5,6498.5,7333,8120,8831,9433.5,9886.5,10185,10393,0,4269,5152,6071,6926,7740,8500,9162,9705,10068,10302,10484]
["NPCC-Ontario","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999949,2189.6217474999958,2189.6217474999921,2189.6217474999903,2189.6217474999917,0,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999944,2189.6217474999949,2189.6217474999958,2189.6217474999921,2189.6217474999903,2189.6217474999917]
["NPCC-Quebec","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,16,42,78,125,181,244,313,386,473,576,576,0,27,56,96,147,206,272,341,420,513,622,622]
["PJM","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,8289.4736842105267,9205.2631578947367,10055.263157894737,10615.78947368421,11115.78947368421,12228.947368421053,12802.631578947368,13547.368421052632,14847.368421052632,15721.052631578947,17639.473684210527,0,8289.4736842105267,9205.2631578947367,10055.263157894737,10615.78947368421,11115.78947368421,12228.947368421053,12802.631578947368,13547.368421052632,14847.368421052632,15721.052631578947,17639.473684210527]
["SERC-C","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,49,49,49,49,49,49,49,49,49,49,49,0,49,49,49,49,49,49,49,49,49,49,49]
["SERC-E","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,549,636,710,774,840,907,975,1045,1116,1187,1258,0,587,668,737,803,870,938,1007,1076,1147,1219,1290]
["SERC-FP","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,1125,1492,1806,2066,2328,2601,2921,3276,3695,4051,4365,0,1215,1577,1856,2093,2360,2639,2966,3325,3745,4106,4424]
["SERC-SE","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["SPP","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,0,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5,62.5]
["Texas RE-ERCOT","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,1531.2368612250004,2031.2368612250004,2531.2368612250002,3031.2368612250002,3531.2368612250002,4031.2368612250002,4531.2368612250002,5031.2368612250002,5531.2368612250002,6031.2368612250002,6531.2368612250002,0,2031.2368612250004,2531.2368612250002,3031.2368612250002,3531.2368612250002,4031.2368612250002,4531.2368612250002,5031.2368612250002,5531.2368612250002,6031.2368612250002,6531.2368612250002,7031.2368612250002]
["WECC-AB","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,115,128,142,155,192,228,264,300,336,396,456,0,115,128,142,155,192,228,264,300,336,396,456]
["WECC-BC","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WECC-CA/MX","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,7785.72757453136,8940.9092136122727,10038.88160020766,11048.351492423804,12096.902862861947,13170.567137112188,14232.328309451304,15393.043798843171,16597.839475193981,17788.831598533237,18929.873721872485,0,8173.7289551654303,9298.1143428356918,10382.845228893642,11379.654624188885,12429.376982198481,13514.982214569041,14589.806356892434,15768.442519818544,17011.302952881699,18204.41796352953,19347.582974177352]
["WECC-WPP","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,2775.5878322637027,3057.1534160558031,3297.8327191715562,3524.7008736571538,3758.1386215531033,4006.9149011708023,4275.5496489824754,4570.1888949760714,4885.5804218445201,5196.1301782279934,3975.4294830158901,0,2862.1904871946231,3138.6872928000753,3363.2745073402757,3592.3471750901244,3829.3958933224908,4083.9151514192426,4360.4093811850953,4665.6676771264501,4989.4020886648486,5290.8370615445556,4052.9852893330876]
["WECC-SRSG","Total Installed BTM Solar PV embedded in load forecast","2022-2032","MW",0,1971.2936324069678,2160.4248702960317,2404.8008925386421,2701.9200983278606,3059.0647430940999,3479.0412510163706,3965.4778916417135,4516.2002616477412,5135.926559655144,5825.0391233269747,6586.9727702563196,0,2012.9401897169205,2223.2911191238713,2479.6950489205092,2792.7059693558804,3166.2463606501033,3603.3919386160537,4106.6438872690769,4676.096981494904,5314.1740774827749,6021.9027877706212,6801.4699091055436]
[null,null,null,null,null,34505.808071500433,39235.08178655048,43900.80178538138,48157.011760859212,52507.136313064562,57459.189021881393,61909.866260509669,66649.881505626981,71999.495686373135,76789.343851613579,80886.500923491942,null,null,null,null,null,null,null,null,null,null,null,75791.098255998339]
[]
[]
[]
[]
[null,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032]
["NERC MW",34505.808071500433,39235.08178655048,43900.80178538138,48157.011760859212,52507.136313064562,57459.189021881393,61909.866260509669,66649.881505626981,71999.495686373135,76789.343851613579,80886.500923491942]